<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - LEDs - Signal LEDs - Chip LED - WL-SMCD&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-01-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SMCD_0603">
<description>&lt;B&gt;WL-SMCD SMT Mono-color Chip LED Diffused 
&lt;/B&gt; &lt;BR&gt;&lt;BR&gt;Size 0603, SMT, 2pins

&lt;BR&gt;1.6x0.8x0.4mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="LED">
<pin name="_" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SMCD_0603" prefix="D">
<description>&lt;b&gt;WL-SMCD SMT Mono-color Chip LED Diffused 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Industrial 0603 platform – 1.6 x 0.8 mm 
&lt;br&gt;Wide viewing angle 140° 
&lt;br&gt;Thin version: 0.4 mm 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Office Automation 
&lt;br&gt;Home appliances 
&lt;br&gt;Industrial equipment 
&lt;br&gt;Front panel backlighting 
&lt;br&gt;Button backlighting 
&lt;br&gt;LCD backlighting 
&lt;br&gt;Navigation backlighting 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o121399v209%20Family_WL-SMCD_0603_thin_0%2C4mm_150060xx55040.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o121399v209%20Family_WL-SMCD_0603_thin_0%2C4mm_150060xx55040.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMCD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SMCD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2024-01-25&lt;br&gt;
&lt;/b&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="WL-SMCD_0603">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="_" pad="1"/>
</connects>
<technologies>
<technology name="_150060AS55040">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150060AS55040?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="605nm"/>
<attribute name="EMITTING-COLOR" value="Amber"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="110mcd"/>
<attribute name="PART-NUMBER" value="150060AS55040"/>
<attribute name="PEAK-WAVELENGTH" value="609nm"/>
<attribute name="VALUE" value="150060AS55040"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
</technology>
<technology name="_150060BS55040">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150060BS55040?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="80mcd"/>
<attribute name="PART-NUMBER" value="150060BS55040"/>
<attribute name="PEAK-WAVELENGTH" value="465nm"/>
<attribute name="VALUE" value="150060BS55040"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
</technology>
<technology name="_150060GS55040">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150060GS55040?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="525nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="430mcd"/>
<attribute name="PART-NUMBER" value="150060GS55040"/>
<attribute name="PEAK-WAVELENGTH" value="520nm"/>
<attribute name="VALUE" value="150060GS55040"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
</technology>
<technology name="_150060RS55040">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150060RS55040?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="624nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="90mcd"/>
<attribute name="PART-NUMBER" value="150060RS55040"/>
<attribute name="PEAK-WAVELENGTH" value="632nm"/>
<attribute name="VALUE" value="150060RS55040"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
</technology>
<technology name="_150060SS55040">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150060SS55040?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="630nm"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="70mcd"/>
<attribute name="PART-NUMBER" value="150060SS55040"/>
<attribute name="PEAK-WAVELENGTH" value="645nm"/>
<attribute name="VALUE" value="150060SS55040"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
</technology>
<technology name="_150060VS55040">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150060VS55040?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="573nm"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="60mcd"/>
<attribute name="PART-NUMBER" value="150060VS55040"/>
<attribute name="PEAK-WAVELENGTH" value="575nm"/>
<attribute name="VALUE" value="150060VS55040"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
</technology>
<technology name="_150060YS55040">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150060YS55040?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="589nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="100mcd"/>
<attribute name="PART-NUMBER" value="150060YS55040"/>
<attribute name="PEAK-WAVELENGTH" value="591nm"/>
<attribute name="VALUE" value="150060YS55040"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
