<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - LEDs - Singnal LEDs &amp; Horticulture LEDs - WL-SMDC&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt;

&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-06-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SMDC_3535">
<description>&lt;b&gt;WL-SMDC SMT Mono-color Ceramic LED Waterclear
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size:3535, SMT
&lt;br&gt;3.45x3.45x0.71mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="WL-SWDC">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SMDC_3535_HORTICULTURE" prefix="D">
<description>&lt;b&gt;WL-SMDC SMT Mono-color Ceramic LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt; SMD LED ceramic package with high efficiency 
&lt;br&gt;Waterclear silicone lense 
&lt;br&gt;High brightness with minimal side emission 
&lt;br&gt;Flexible coupling with secondary optic 
&lt;br&gt;Narrow viewing angle: 60° 
&lt;br&gt;Moisture Sensitivity Level: 1 
&lt;br&gt;Electrically neutral thermal path 
&lt;br&gt;Low thermal resistance: 125°C / 150°C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;&lt;br&gt;&lt;/b&gt; Architectural LED lighting indoor 
&lt;br&gt;Entertainment and stage lighting 
&lt;br&gt;Indoor smart lights 
&lt;br&gt;Horticultural lighting 
&lt;br&gt;Aquarium lighting 
&lt;br&gt;Traffic and signal lights 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o121137v209%20Family_WL-SMDC_3535_150353xx74500.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o121137v209%20Family_WL-SMDC_3535_150353xx74500.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMDC_HORTICULTURE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMDC_HORTICULTURE&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Ella Wu, 2022-06-18&lt;br&gt;
&lt;/b&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SWDC"/>
</gates>
<devices>
<device name="" package="WL-SMDC_3535">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_150353DS74500">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150353DS74500?ae"/>
<attribute name="EMITTING-COLOR" value="Deep Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="PART-NUMBER" value="150353DS74500"/>
<attribute name="PEAK-WAVELENGTH" value="450nm"/>
<attribute name="RADIANT-FLUX" value="600nW"/>
<attribute name="VALUE" value="150353DS74500"/>
<attribute name="VIEWING-ANGLE" value="125°"/>
</technology>
<technology name="_150353FS74500">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150353FS74500?ae"/>
<attribute name="EMITTING-COLOR" value="Far Red"/>
<attribute name="FORWARD-VOLTAGE" value="1.8V"/>
<attribute name="PART-NUMBER" value="150353FS74500"/>
<attribute name="PEAK-WAVELENGTH" value="730nm"/>
<attribute name="RADIANT-FLUX" value="330mW"/>
<attribute name="VALUE" value="150353FS74500"/>
<attribute name="VIEWING-ANGLE" value="125°"/>
</technology>
<technology name="_150353HS74500">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150353HS74500?ae"/>
<attribute name="EMITTING-COLOR" value="Hyper Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.4V"/>
<attribute name="PART-NUMBER" value="150353HS74500"/>
<attribute name="PEAK-WAVELENGTH" value="660nm"/>
<attribute name="RADIANT-FLUX" value="400mW"/>
<attribute name="VALUE" value="150353HS74500"/>
<attribute name="VIEWING-ANGLE" value="125°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMDC_3535" prefix="D">
<description>&lt;b&gt;WL-SMDC SMT Mono-color Ceramic LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt; SMD LED ceramic package with high efficiency 
&lt;br&gt;Waterclear silicone lense 
&lt;br&gt;High brightness with minimal side emission 
&lt;br&gt;Flexible coupling with secondary optic 
&lt;br&gt;Narrow viewing angle: 60° 
&lt;br&gt;Moisture Sensitivity Level: 1 
&lt;br&gt;Electrically neutral thermal path 
&lt;br&gt;Low thermal resistance: 125°C / 150°C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;&lt;br&gt;&lt;/b&gt; Architectural LED lighting indoor 
&lt;br&gt;Entertainment and stage lighting 
&lt;br&gt;Indoor smart lights 
&lt;br&gt;Horticultural lighting 
&lt;br&gt;Aquarium lighting 
&lt;br&gt;Traffic and signal lights 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14907v209%20Family_WL-SMDC_3535.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14907v209%20Family_WL-SMDC_3535.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMDC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMDC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Ella Wu,2022-06-18&lt;br&gt;
&lt;/b&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SWDC"/>
</gates>
<devices>
<device name="" package="WL-SMDC_3535">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_150353BS74500">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150353BS74500?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="460nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-FLUX" value="25lm"/>
<attribute name="PART-NUMBER" value="150353BS74500"/>
<attribute name="PEAK-WAVELENGTH" value="455nm"/>
<attribute name="VALUE" value="150353BS74500"/>
<attribute name="VIEWING-ANGLE" value="125°"/>
</technology>
<technology name="_150353GS74500">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150353GS74500?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="525nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3.4V"/>
<attribute name="LUMINOUS-FLUX" value="85lm"/>
<attribute name="PART-NUMBER" value="150353GS74500"/>
<attribute name="PEAK-WAVELENGTH" value="520nm"/>
<attribute name="VALUE" value="150353GS74500"/>
<attribute name="VIEWING-ANGLE" value="125°"/>
</technology>
<technology name="_150353RS74500">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150353RS74500?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="LUMINOUS-FLUX" value="55lm"/>
<attribute name="PART-NUMBER" value="150353RS74500"/>
<attribute name="PEAK-WAVELENGTH" value="635nm"/>
<attribute name="VALUE" value="150353RS74500"/>
<attribute name="VIEWING-ANGLE" value="125°"/>
</technology>
<technology name="_150353YS74500">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150353YS74500?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="LUMINOUS-FLUX" value="50lm"/>
<attribute name="PART-NUMBER" value="150353YS74500"/>
<attribute name="PEAK-WAVELENGTH" value="593nm"/>
<attribute name="VALUE" value="150353YS74500"/>
<attribute name="VIEWING-ANGLE" value="125°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
