<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - Ultraviolet - WL-SUMW&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SUMW_3535_15335327CA554">
<description>&lt;b&gt;WL-SUMW SMT Ultraviolet Ceramic Waterclear
&lt;br&gt;&lt;br&gt;&lt;/b&gt;3535 UV-C, SMT, 3pins
&lt;br&gt;LXWXH=3.7X3.7X1.8mm</description>
</package>
<package name="WL-SUMW_3535_153353XXAA350">
<description>&lt;B&gt;WL-SUMW SMT Ultraviolet Ceramic Waterclear
&lt;BR&gt;&lt;/B&gt;&lt;BR&gt;Size: 3535, SMT, 3pins
&lt;BR&gt;L X W X H = 3.4mm X 3.4mm X 2.1mm</description>
</package>
<package name="WL-SUMW_3535_15335327CA452">
<description>&lt;b&gt;WL-SUMW SMT Ultraviolet Ceramic Waterclear
&lt;br&gt;&lt;br&gt;&lt;/b&gt;3535 UV-C, SMT, 3pins
&lt;br&gt;LXWXH=3.7X3.7X1.8mm</description>
</package>
<package name="WL-SUMW_3535_153353XXBA25X">
<description>&lt;B&gt;WL-SUMW SMT Ultraviolet Ceramic Waterclear
&lt;BR&gt;&lt;/B&gt;&lt;BR&gt;Size: 3535 UV-C, SMT, 3pins
&lt;BR&gt;L X W X H = 3.55mm X 3.55mm X 1.62mm</description>
</package>
</packages>
<symbols>
<symbol name="WL-SUMW">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SUMW_3535_UV-A" prefix="D">
<description>&lt;b&gt; WL-SUMW SMT Ultraviolet Ceramic Waterclear 
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;

&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High power output UV LEDs
&lt;br&gt;Low thermal resistance
&lt;br&gt;Peak wavelengths: 275, 365, 385, 395, 405 nm
&lt;br&gt;Standard soldering pad footprint
&lt;/b&gt;&lt;br&gt;

&lt;b&gt;&lt;br&gt;Applications
&lt;br&gt;&lt;br&gt;UV-A:
&lt;/b&gt;&lt;br&gt;UV-Curing
&lt;br&gt;Printing / coating Adhesive
&lt;br&gt;Counterfeit detection
&lt;br&gt;Security Forensic
&lt;br&gt;Special lighting

           
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o81007v209%20WL-SUMW_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o81007v209%20WL-SUMW_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SUMW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WL-SUMW&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

Updated by Ella 2025-03-11&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SUMW"/>
</gates>
<devices>
<device name="_153353XXAA350" package="WL-SUMW_3535_153353XXAA350">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name="_15335337AA350">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15335337AA350?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3.8V"/>
<attribute name="PART-NUMBER" value="15335337AA350"/>
<attribute name="PEAK-WAVELENGTH" value="365nm"/>
<attribute name="RADIANT-FLUX-MAX" value="1300mW"/>
<attribute name="RADIANT-FLUX-MIN" value="700mW"/>
<attribute name="VALUE" value="15335337AA350"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
<technology name="_15335338AA350">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15335338AA350?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3.5V"/>
<attribute name="PART-NUMBER" value="15335338AA350"/>
<attribute name="PEAK-WAVELENGTH" value="385nm"/>
<attribute name="RADIANT-FLUX-MAX" value="1300mW"/>
<attribute name="RADIANT-FLUX-MIN" value="800mW"/>
<attribute name="VALUE" value="15335338AA350"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
<technology name="_15335339AA350">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15335339AA350?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3.5V"/>
<attribute name="PART-NUMBER" value="15335339AA350"/>
<attribute name="PEAK-WAVELENGTH" value="395nm"/>
<attribute name="RADIANT-FLUX-MAX" value="1300mW"/>
<attribute name="RADIANT-FLUX-MIN" value="800mW"/>
<attribute name="VALUE" value="15335339AA350"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
<technology name="_15335340AA350">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15335340AA350?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3.5V"/>
<attribute name="PART-NUMBER" value="15335340AA350"/>
<attribute name="PEAK-WAVELENGTH" value="405nm"/>
<attribute name="RADIANT-FLUX-MAX" value="1300mW"/>
<attribute name="RADIANT-FLUX-MIN" value="800mW"/>
<attribute name="VALUE" value="15335340AA350"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SUMW_3535_UV-C" prefix="D">
<description>&lt;b&gt; WL-SUMW SMT Ultraviolet Ceramic Waterclear 
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;

&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High power output UV LEDs
&lt;br&gt;Low thermal resistance
&lt;br&gt;Peak wavelengths: 275, 365, 385, 395, 405 nm
&lt;br&gt;Standard soldering pad footprint
&lt;/b&gt;&lt;br&gt;

&lt;b&gt;&lt;br&gt;Applications
&lt;br&gt;&lt;br&gt;UV-C:
&lt;/b&gt;&lt;br&gt;Sterilization
&lt;br&gt;Surface disinfection
&lt;br&gt;Water purification
&lt;br&gt;Air purification

           
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o81007v209%20WL-SUMW_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o81007v209%20WL-SUMW_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SUMW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WL-SUMW&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

Updated by Ella 2025-03-11&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SUMW"/>
</gates>
<devices>
<device name="_153353XXBA25X" package="WL-SUMW_3535_153353XXBA25X">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name="_15335327BA250">
<attribute name="CHIP-TECHNOLOGY" value="AlGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15335327BA250?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="6.5V"/>
<attribute name="PART-NUMBER" value="15335327BA250"/>
<attribute name="PEAK-WAVELENGTH" value="275nm"/>
<attribute name="RADIANT-FLUX-MIN" value="1.5mW"/>
<attribute name="RADIANT-FLUX-TYP" value="3mW"/>
<attribute name="VALUE" value="15335327BA250"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_15335327BA252">
<attribute name="CHIP-TECHNOLOGY" value="AlGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15335327BA252?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="6V"/>
<attribute name="PART-NUMBER" value="15335327BA252"/>
<attribute name="PEAK-WAVELENGTH" value="275nm"/>
<attribute name="RADIANT-FLUX-MIN" value="8mW"/>
<attribute name="RADIANT-FLUX-TYP" value="15mW"/>
<attribute name="VALUE" value="15335327BA252"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
<device name="_15335327CA452" package="WL-SUMW_3535_15335327CA452">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name="_15335327CA452">
<attribute name="CHIP-TECHNOLOGY" value="AlGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15335327CA452?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="6V"/>
<attribute name="PART-NUMBER" value="15335327CA452"/>
<attribute name="PEAK-WAVELENGTH" value="275nm"/>
<attribute name="RADIANT-FLUX-MIN" value="13mW"/>
<attribute name="RADIANT-FLUX-TYP" value="20mW"/>
<attribute name="VALUE" value="15335327CA452"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
<device name="_15335327CA554" package="WL-SUMW_3535_15335327CA554">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name="_15335327CA554">
<attribute name="CHIP-TECHNOLOGY" value="AlGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15335327CA554?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="6V"/>
<attribute name="PART-NUMBER" value="15335327CA554"/>
<attribute name="PEAK-WAVELENGTH" value="275nm"/>
<attribute name="RADIANT-FLUX-MIN" value="40mW"/>
<attribute name="RADIANT-FLUX-TYP" value="50mW"/>
<attribute name="VALUE" value="15335327CA554"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
