<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - Ultraviolet - WL-SUTW&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt;

&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-06-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SUTW_2835_153283367A212">
<description>&lt;b&gt;WL-SUTW SMT Ultraviolet Top LED Waterclear 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size:2835, SMT, 2Pins
&lt;br&gt;LXWXL = 3.5mmX2.8mmX0.7mm</description>
</package>
<package name="WL-SUTW_2835_153283XX7A212">
<description>&lt;b&gt;WL-SUTW SMT Ultraviolet Top LED Waterclear 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size:2835, SMT, 2Pins
&lt;br&gt;LXWXL = 3.5mmX2.8mmX0.7mm</description>
</package>
</packages>
<symbols>
<symbol name="WL-SUTW">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SUTW_2835" prefix="D">
<description>&lt;b&gt; WL-SUTW SMT Ultraviolet Top LED Waterclear 
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;

&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;UV-A emitting LEDs
&lt;br&gt;Peak wavelengths: 365, 385, 395, 405 nm
&lt;br&gt;Standard 2835 PLCC 2 package
&lt;br&gt;Flat package
&lt;br&gt;Viewing angle 120°
&lt;/b&gt;&lt;br&gt;

&lt;b&gt;&lt;br&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Horticulture
&lt;br&gt;UV curing
&lt;br&gt;Sensing applications
&lt;br&gt;Counterfeit detection

           
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o532286v209%20WL-SUTW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o532286v209%20WL-SUTW.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SUTW"&gt;www.we-online.com/catalog/WL-SUTW&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

Created by Ella Wu 2022-05-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SUTW"/>
</gates>
<devices>
<device name="_153283367A212" package="WL-SUTW_2835_153283367A212">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/153283367A212?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3.6V"/>
<attribute name="PART-NUMBER" value="153283367A212"/>
<attribute name="PEAK-WAVELENGTH" value="365nm"/>
<attribute name="RADIANT-FLUX-MAX" value="90nW"/>
<attribute name="RADIANT-FLUX-MIN" value="30nW"/>
<attribute name="RADIANT-FLUX-TYP" value="50nW"/>
<attribute name="VALUE" value="153283367A212"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
<device name="_153283XX7A212" package="WL-SUTW_2835_153283XX7A212">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name="_153283387A212">
<attribute name="CHIP-TECHNOLOGY" value="GaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/153283387A212?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3.4V"/>
<attribute name="PART-NUMBER" value="153283387A212"/>
<attribute name="PEAK-WAVELENGTH" value="385nm"/>
<attribute name="RADIANT-FLUX-MAX" value="130nW"/>
<attribute name="RADIANT-FLUX-MIN" value="50nW"/>
<attribute name="RADIANT-FLUX-TYP" value="90nW"/>
<attribute name="VALUE" value="153283387A212"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_153283397A212">
<attribute name="CHIP-TECHNOLOGY" value="GaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/153283397A212?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3.4V"/>
<attribute name="PART-NUMBER" value="153283397A212"/>
<attribute name="PEAK-WAVELENGTH" value="395nm"/>
<attribute name="RADIANT-FLUX-MAX" value="190nW"/>
<attribute name="RADIANT-FLUX-MIN" value="80nW"/>
<attribute name="RADIANT-FLUX-TYP" value="140nW"/>
<attribute name="VALUE" value="153283397A212"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_153283407A212">
<attribute name="CHIP-TECHNOLOGY" value="GaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/153283407A212?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3.4V"/>
<attribute name="PART-NUMBER" value="153283407A212"/>
<attribute name="PEAK-WAVELENGTH" value="405nm"/>
<attribute name="RADIANT-FLUX-MAX" value="190nW"/>
<attribute name="RADIANT-FLUX-MIN" value="80nW"/>
<attribute name="RADIANT-FLUX-TYP" value="140nW"/>
<attribute name="VALUE" value="153283407A212"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
