<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - LEDs - General Lighting - WL-SWTC&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt;

&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-06-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SWTC_3535">
<description>&lt;b&gt;WL-SWTC SMT White Top view Ceramic LED
&lt;/b&gt;&lt;br&gt;&lt;br&gt;  Size 3535, SMT
&lt;br&gt;3.45x3.45x0.71mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="WL-SWTC">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SWTC_3535" prefix="D">
<description>&lt;b&gt; WL-SWTC SMT White Top view Ceramic LED 
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Fast switching
&lt;/b&gt;&lt;br&gt;No IR radiation
&lt;/b&gt;&lt;br&gt;High brightness
&lt;/b&gt;&lt;br&gt;Minimal side emission
&lt;/b&gt;&lt;br&gt;Waterclear silicone lens
&lt;/b&gt;&lt;br&gt;Top view
&lt;/b&gt;&lt;br&gt;Flexible coupling with secondary optic
&lt;/b&gt;&lt;br&gt;Various color temperatures
&lt;/b&gt;&lt;br&gt;Compact footprint
&lt;/b&gt;&lt;br&gt;Thermal resistance junction to solder point: 8 °K/W
&lt;/b&gt;&lt;br&gt;LED junction temperature: 150 °C
&lt;/b&gt;&lt;br&gt;Moisture Sensitivity Level: 2

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;&lt;br&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Indoor lighting: Spot light, Down light
&lt;/b&gt;&lt;br&gt;Outdoor lighting: Street light, Security light, Tunnel light, Parking lots light
&lt;/b&gt;&lt;br&gt;Industrial lighting: High-bay light, Low-bay light
&lt;/b&gt;&lt;br&gt;Consumer lighting: Torch light
&lt;/b&gt;&lt;br&gt;Agricultural equipment lighting
&lt;/b&gt;&lt;br&gt;Signal and symbol luminaries
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14909v209%20Family_WL-SWTC_3535.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14909v209%20Family_WL-SWTC_3535.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SWTC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SWTC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SWTC"/>
</gates>
<devices>
<device name="" package="WL-SWTC_3535">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_158353040">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="COLOR-RENDERING-INDEX" value=" 75 "/>
<attribute name="CORRELATED-COLOR-TEMPERATURE" value="4000K"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/158353040?ae"/>
<attribute name="EMITTING-COLOR" value="Moonlight"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-FLUX" value="121lm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 158353040 "/>
<attribute name="VALUE" value=" 158353040 "/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_158353050">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="COLOR-RENDERING-INDEX" value=" 70 "/>
<attribute name="CORRELATED-COLOR-TEMPERATURE" value="5000K"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/158353050?ae"/>
<attribute name="EMITTING-COLOR" value="Daylight"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-FLUX" value="135lm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 158353050 "/>
<attribute name="VALUE" value=" 158353050 "/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_158353060">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="COLOR-RENDERING-INDEX" value=" 70 "/>
<attribute name="CORRELATED-COLOR-TEMPERATURE" value="6000K"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/158353060?ae"/>
<attribute name="EMITTING-COLOR" value="Cool White"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-FLUX" value="135lm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 158353060 "/>
<attribute name="VALUE" value=" 158353060 "/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
