<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Infrared - Infrared LEDs - WL-TIRW&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-12-08&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-TIRW_3MM">
<description>&lt;b&gt;WL-TIRW&lt;/b&gt;&lt;br&gt; THT Infrared Round Waterclear,3mm without stopper</description>
</package>
<package name="WL-TIRW_5MM">
<description>&lt;b&gt;WL-TIRW&lt;/b&gt;&lt;br&gt; THT Infrared Round Waterclear,5mm without stopper</description>
</package>
</packages>
<symbols>
<symbol name="LED">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-TIRW_5MM" prefix="D">
<description>&lt;b&gt;WL-TIRW THT Infrared Round Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Infrared Emitter 
&lt;br&gt;Very High Radiant Intensity 
&lt;br&gt;standard size 3mm and 5mm 
&lt;br&gt;Fast switching 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Status light 
&lt;br&gt;Sensor Technology 
&lt;br&gt;Distance measurement 
&lt;br&gt;Remote control 
&lt;br&gt;Smoke detectors 
&lt;br&gt;Data Transmission 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o82201v209%20Family_WL-TIRW_3mm.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o82201v209%20Family_WL-TIRW_3mm.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-TIRW/"&gt;https://www.we-online.com/catalog/en/WL-TIRW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Ella Wu 2021-12-08&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="_WITHOUTSTOPPER" package="WL-TIRW_5MM">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15400585A3590">
<attribute name="CENTROID-WAVELENGTH" value="845nm"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15400585A3590.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="FORWARD-VOLTAGE" value="1.5V"/>
<attribute name="PART-NUMBER" value="15400585A3590"/>
<attribute name="PEAK-WAVELENGTH" value="850nm"/>
<attribute name="RADIANT-INTENSITY" value="85mW/sr"/>
<attribute name="VALUE" value="15400585A3590"/>
<attribute name="VIEWING-ANGLE" value="35°"/>
</technology>
<technology name="_15400594A3590">
<attribute name="CENTROID-WAVELENGTH" value="940nm"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15400594A3590.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="FORWARD-VOLTAGE" value="1.3V"/>
<attribute name="PART-NUMBER" value="15400594A3590"/>
<attribute name="PEAK-WAVELENGTH" value="940nm"/>
<attribute name="RADIANT-INTENSITY" value="30mW/sr"/>
<attribute name="VALUE" value="15400594A3590"/>
<attribute name="VIEWING-ANGLE" value="35°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-TIRW_3MM" prefix="D">
<description>&lt;b&gt;WL-TIRW THT Infrared Round Waterclear
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Infrared Emitter 
&lt;br&gt;Very High Radiant Intensity 
&lt;br&gt;standard size 3mm and 5mm 
&lt;br&gt;Fast switching 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Status light 
&lt;br&gt;Sensor Technology 
&lt;br&gt;Distance measurement 
&lt;br&gt;Remote control 
&lt;br&gt;Smoke detectors 
&lt;br&gt;Data Transmission 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o82201v209%20Family_WL-TIRW_3mm.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o82201v209%20Family_WL-TIRW_3mm.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-TIRW/"&gt;https://www.we-online.com/catalog/en/WL-TIRW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun,Shan,2020-03-24&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="_WITHOUTSTOPPER" package="WL-TIRW_3MM">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15400385A3590">
<attribute name="CENTROID-WAVELENGTH" value="845nm"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15400385A3590.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="FORWARD-VOLTAGE" value="1.5V"/>
<attribute name="PART-NUMBER" value="15400385A3590"/>
<attribute name="PEAK-WAVELENGTH" value="850nm"/>
<attribute name="RADIANT-INTENSITY" value="60mW/sr"/>
<attribute name="VALUE" value="15400385A3590"/>
<attribute name="VIEWING-ANGLE" value="35°"/>
</technology>
<technology name="_15400394A3590">
<attribute name="CENTROID-WAVELENGTH" value="940nm"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15400394A3590.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="FORWARD-VOLTAGE" value="1.3V"/>
<attribute name="PART-NUMBER" value="15400394A3590"/>
<attribute name="PEAK-WAVELENGTH" value="940nm"/>
<attribute name="RADIANT-INTENSITY" value="75mW/sr"/>
<attribute name="VALUE" value="15400394A3590"/>
<attribute name="VIEWING-ANGLE" value="35°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
