<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - REDCUBE - REDCUBE PRESS-FIT - WP-BUCF&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-09-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WP-BUCF_7460408">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M5 , 12pins
&lt;br&gt;Max Height = 6mm</description>
</package>
<package name="WP-BUCF_7461148">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M2.5 , 8pins
&lt;br&gt;Max Height =6mm</description>
</package>
<package name="WP-BUCF_7461059_HAL">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M6 , 16pins
&lt;br&gt;Max Height = 13.5mm</description>
</package>
<package name="WP-BUCF_7460408_HAL">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M5 , 12pins
&lt;br&gt;Max Height = 6mm</description>
</package>
<package name="WP-BUCF_7461059">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M6 , 16pins
&lt;br&gt;Max Height = 13.5mm</description>
</package>
<package name="WP-BUCF_7461086">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M4 , 12pins
&lt;br&gt;Max Height = 6mm</description>
</package>
<package name="WP-BUCF_7461148_HAL">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M2.5 , 8pins
&lt;br&gt;Max Height =6mm</description>
</package>
<package name="WP-BUCF_7461060">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M10 , 20pins
&lt;br&gt;Max Height = 17.5mm</description>
</package>
<package name="WP-BUCF_7461090_HAL">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M8 , 20pins
&lt;br&gt;Max Height = 13.5mm</description>
</package>
<package name="WP-BUCF_7461090">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M8 , 20pins
&lt;br&gt;Max Height = 13.5mm</description>
</package>
<package name="WP-BUCF_7461086_HAL">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M4 , 12pins
&lt;br&gt;Max Height = 6mm</description>
</package>
<package name="WP-BUCF_7461060_HAL">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M10 , 20pins
&lt;br&gt;Max Height = 17.5mm</description>
</package>
</packages>
<symbols>
<symbol name="WP-BUCF">
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WP-BUCF" prefix="MP">
<description>&lt;b&gt;WP-BUCF Internal thread, circumference
&lt;br&gt;
&lt;br&gt; Applications&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High current Wire-to-Board connections up to 500 A
&lt;br&gt;Mounting of copper bars on PCBs
&lt;br&gt;Installation of laminated fuses
&lt;br&gt;Suitable for rough environmental conditions
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55764v209%20WP-BUCF_Family.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55764v209%20WP-BUCF_Family.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WP-BUCF_CIRCUMFERENCE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/katalog/em/WP-BUCF_CIRCUMFERENCE&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-29
&lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WP-BUCF"/>
</gates>
<devices>
<device name="_7461148" package="WP-BUCF_7461148">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461148?ae"/>
<attribute name="IR" value="130A"/>
<attribute name="PART-NUMBER" value=" 7461148 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="THREAD" value="M2.5"/>
<attribute name="VALUE" value=" 7461148 "/>
</technology>
</technologies>
</device>
<device name="_7461148_HAL" package="WP-BUCF_7461148_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461148?ae"/>
<attribute name="IR" value="130A"/>
<attribute name="PART-NUMBER" value=" 7461148 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="THREAD" value="M2.5"/>
<attribute name="VALUE" value=" 7461148 "/>
</technology>
</technologies>
</device>
<device name="_7460408" package="WP-BUCF_7460408">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7460408?ae"/>
<attribute name="IR" value="175A"/>
<attribute name="PART-NUMBER" value=" 7460408 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="THREAD" value="M5"/>
<attribute name="VALUE" value=" 7460408 "/>
</technology>
</technologies>
</device>
<device name="_7460408_HAL" package="WP-BUCF_7460408_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7460408?ae"/>
<attribute name="IR" value="175A"/>
<attribute name="PART-NUMBER" value=" 7460408 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="THREAD" value="M5"/>
<attribute name="VALUE" value=" 7460408 "/>
</technology>
</technologies>
</device>
<device name="_7461059" package="WP-BUCF_7461059">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461059?ae"/>
<attribute name="IR" value="240A"/>
<attribute name="PART-NUMBER" value=" 7461059 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="THREAD" value="M6"/>
<attribute name="VALUE" value=" 7461059 "/>
</technology>
</technologies>
</device>
<device name="_7461059_HAL" package="WP-BUCF_7461059_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461059?ae"/>
<attribute name="IR" value="240A"/>
<attribute name="PART-NUMBER" value=" 7461059 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="THREAD" value="M6"/>
<attribute name="VALUE" value=" 7461059 "/>
</technology>
</technologies>
</device>
<device name="_7461090" package="WP-BUCF_7461090">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461090?ae"/>
<attribute name="IR" value="350A"/>
<attribute name="PART-NUMBER" value=" 7461090 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="THREAD" value="M8"/>
<attribute name="VALUE" value=" 7461090 "/>
</technology>
</technologies>
</device>
<device name="_7461090_HAL" package="WP-BUCF_7461090_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461090?ae"/>
<attribute name="IR" value="350A"/>
<attribute name="PART-NUMBER" value=" 7461090 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="THREAD" value="M8"/>
<attribute name="VALUE" value=" 7461090 "/>
</technology>
</technologies>
</device>
<device name="_7461086" package="WP-BUCF_7461086">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461086?ae"/>
<attribute name="IR" value="175A"/>
<attribute name="PART-NUMBER" value=" 7461086 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="THREAD" value="M4"/>
<attribute name="VALUE" value=" 7461086 "/>
</technology>
</technologies>
</device>
<device name="_7461086_HAL" package="WP-BUCF_7461086_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461086?ae"/>
<attribute name="IR" value="175A"/>
<attribute name="PART-NUMBER" value=" 7461086 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="THREAD" value="M4"/>
<attribute name="VALUE" value=" 7461086 "/>
</technology>
</technologies>
</device>
<device name="_7461060_HAL" package="WP-BUCF_7461060_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461060?ae"/>
<attribute name="IR" value="350A"/>
<attribute name="PART-NUMBER" value=" 7461060 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="THREAD" value="M10"/>
<attribute name="VALUE" value=" 7461060 "/>
</technology>
</technologies>
</device>
<device name="_7461060" package="WP-BUCF_7461060">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461060?ae"/>
<attribute name="IR" value="350A"/>
<attribute name="PART-NUMBER" value=" 7461060 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="THREAD" value="M10"/>
<attribute name="VALUE" value=" 7461060 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
