<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - REDCUBE - REDCUBE PRESS-FIT - WP-BUFU&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-09-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WP-BUFU_7461061">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M10 , 36pins
&lt;br&gt;Max Height = 17.5mm</description>
</package>
<package name="WP-BUFU_7461061_HAL">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M10 , 36pins
&lt;br&gt;Max Height = 17.5mm</description>
</package>
<package name="WP-BUFU_7461093">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M3 , 9pins
&lt;br&gt;Max Height = 6mm</description>
</package>
<package name="WP-BUFU_7461095">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M4 , 16pins
&lt;br&gt;Max Height = 7mm</description>
</package>
<package name="WP-BUFU_7461093_HAL">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M3 , 9pins
&lt;br&gt;Max Height = 6mm</description>
</package>
<package name="WP-BUFU_7462810">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M3 , 4pins
&lt;br&gt;Max Height = 7mm</description>
</package>
<package name="WP-BUFU_7462810_HAL">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M3 , 4pins
&lt;br&gt;Max Height = 7mm</description>
</package>
<package name="WP-BUFU_7461097_HAL">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M6 , 16pins
&lt;br&gt;Max Height = 10.5mm</description>
</package>
<package name="WP-BUFU_7461097">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M6 , 16pins
&lt;br&gt;Max Height = 10.5mm</description>
</package>
<package name="WP-BUFU_7461099_HAL">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M8 , 25pins
&lt;br&gt;Max Height = 13.5mm</description>
</package>
<package name="WP-BUFU_7461147_HAL">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M5 , 16pins
&lt;br&gt;Max Height = 7mm</description>
</package>
<package name="WP-BUFU_7461099">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M8 , 25pins
&lt;br&gt;Max Height = 13.5mm</description>
</package>
<package name="WP-BUFU_7461095_HAL">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL
&lt;br&gt;Thread M4 , 16pins
&lt;br&gt;Max Height = 7mm</description>
</package>
<package name="WP-BUFU_7461147">
<description>&lt;b&gt;WP-BUFU Internal thread, full plain
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M5 , 16pins
&lt;br&gt;Max Height = 7mm</description>
</package>
</packages>
<symbols>
<symbol name="WP-BUFU">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PRESSFIT">
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WP-BUFU" prefix="MP">
<description>&lt;b&gt; WP-BUFU Internal thread, full plain
&lt;br&gt;
&lt;br&gt;  Applications&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Using the Press-Fit Elements, currents of up to approx. 300A can be transferred to the PCB.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Material Brass 
&lt;br&gt;Surface Tin 
&lt;br&gt;Execution Press-Fit 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -55 up to +150 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Bulk 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55767v209%20Family_WP-BUFU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55767v209%20Family_WP-BUFU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WP-BUFU_FULL_PLAIN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/katalog/em/WP-BUFU_FULL_PLAIN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-29
&lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="PRESSFIT"/>
</gates>
<devices>
<device name="_7461061" package="WP-BUFU_7461061">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461061?ae"/>
<attribute name="IR" value="350A"/>
<attribute name="PART-NUMBER" value=" 7461061 "/>
<attribute name="PINS" value=" 36 "/>
<attribute name="THREAD" value="M10"/>
<attribute name="VALUE" value=" 7461061 "/>
</technology>
</technologies>
</device>
<device name="_7461061_HAL" package="WP-BUFU_7461061_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461061?ae"/>
<attribute name="IR" value="350A"/>
<attribute name="PART-NUMBER" value=" 7461061 "/>
<attribute name="PINS" value=" 36 "/>
<attribute name="THREAD" value="M10"/>
<attribute name="VALUE" value=" 7461061 "/>
</technology>
</technologies>
</device>
<device name="_7462810" package="WP-BUFU_7462810">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7462810?ae"/>
<attribute name="IR" value="70A"/>
<attribute name="PART-NUMBER" value=" 7462810 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="THREAD" value="M3"/>
<attribute name="VALUE" value=" 7462810 "/>
</technology>
</technologies>
</device>
<device name="_7462810_HAL" package="WP-BUFU_7462810_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7462810?ae"/>
<attribute name="IR" value="70A"/>
<attribute name="PART-NUMBER" value=" 7462810 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="THREAD" value="M3"/>
<attribute name="VALUE" value=" 7462810 "/>
</technology>
</technologies>
</device>
<device name="_7461093" package="WP-BUFU_7461093">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461093?ae"/>
<attribute name="IR" value="130A"/>
<attribute name="PART-NUMBER" value=" 7461093 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="THREAD" value="M3"/>
<attribute name="VALUE" value=" 7461093 "/>
</technology>
</technologies>
</device>
<device name="_7461093_HAL" package="WP-BUFU_7461093_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461093?ae"/>
<attribute name="IR" value="130A"/>
<attribute name="PART-NUMBER" value=" 7461093 "/>
<attribute name="PINS" value=" 9 "/>
<attribute name="THREAD" value="M3"/>
<attribute name="VALUE" value=" 7461093 "/>
</technology>
</technologies>
</device>
<device name="_7461095" package="WP-BUFU_7461095">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461095?ae"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 7461095 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="THREAD" value="M4"/>
<attribute name="VALUE" value=" 7461095 "/>
</technology>
</technologies>
</device>
<device name="_7461095_HAL" package="WP-BUFU_7461095_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461095?ae"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 7461095 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="THREAD" value="M4"/>
<attribute name="VALUE" value=" 7461095 "/>
</technology>
</technologies>
</device>
<device name="_7461097" package="WP-BUFU_7461097">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461097?ae"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 7461097 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="THREAD" value="M6"/>
<attribute name="VALUE" value=" 7461097 "/>
</technology>
</technologies>
</device>
<device name="_7461097_HAL" package="WP-BUFU_7461097_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461097?ae"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 7461097 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="THREAD" value="M6"/>
<attribute name="VALUE" value=" 7461097 "/>
</technology>
</technologies>
</device>
<device name="_7461099" package="WP-BUFU_7461099">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461099?ae"/>
<attribute name="IR" value="250A"/>
<attribute name="PART-NUMBER" value=" 7461099 "/>
<attribute name="PINS" value=" 25 "/>
<attribute name="THREAD" value="M8"/>
<attribute name="VALUE" value=" 7461099 "/>
</technology>
</technologies>
</device>
<device name="_7461099_HAL" package="WP-BUFU_7461099_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461099?ae"/>
<attribute name="IR" value="250A"/>
<attribute name="PART-NUMBER" value=" 7461099 "/>
<attribute name="PINS" value=" 25 "/>
<attribute name="THREAD" value="M8"/>
<attribute name="VALUE" value=" 7461099 "/>
</technology>
</technologies>
</device>
<device name="_7461147" package="WP-BUFU_7461147">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461147?ae"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 7461147 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="THREAD" value="M5"/>
<attribute name="VALUE" value=" 7461147 "/>
</technology>
</technologies>
</device>
<device name="_7461147_HAL" package="WP-BUFU_7461147_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7461147?ae"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 7461147 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="THREAD" value="M5"/>
<attribute name="VALUE" value=" 7461147 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
