<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - REDCUBE Terminals - REDCUBE PRESS-FIT - PRESS-FIT right angled - WP-RAFE&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-12-01&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WP-RAFE_74622103">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M3 , 6pins
&lt;br&gt;Max Height = 14mm</description>
</package>
<package name="WP-RAFE_74622105_HAL">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL 
&lt;br&gt;Thread M5 , 12pins
&lt;br&gt;Max Height = 14mm</description>
</package>
<package name="WP-RAFE_74622103_HAL">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL 
&lt;br&gt;Thread M3 , 6pins
&lt;br&gt;Max Height = 14mm</description>
</package>
<package name="WP-RAFE_74622105">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M5 , 12pins
&lt;br&gt;Max Height = 14mm</description>
</package>
<package name="WP-RAFE_74622106">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M6 , 20pins
&lt;br&gt;Max Height = 20mm</description>
</package>
<package name="WP-RAFE_74622108_HAL">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL 
&lt;br&gt;Thread M8 , 20pins
&lt;br&gt;Max Height = 20mm</description>
</package>
<package name="WP-RAFE_74622108">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M8 , 20pins
&lt;br&gt;Max Height = 20mm</description>
</package>
<package name="WP-RAFE_74622106_HAL">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M6 , 20pins
&lt;br&gt;Max Height = 20mm</description>
</package>
<package name="WP-RAFE_74622104_HAL">
<description>&lt;b&gt;WP-RAFEU 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for HAL 
&lt;br&gt;Thread M4 , 12pins
&lt;br&gt;Max Height = 14mm</description>
</package>
<package name="WP-RAFE_74622104">
<description>&lt;b&gt;WP-RAFE 90°, 2-rows, full, edge
&lt;br&gt;&lt;/b&gt;Drill hole specification for chemical surfaces
&lt;br&gt;Thread M4 , 12pins
&lt;br&gt;Max Height = 14mm</description>
</package>
</packages>
<symbols>
<symbol name="WP-RAFE">
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WP-RAFE" prefix="MP">
<description>&lt;b&gt;WP-RAFE REDCUBE PRESS-FIT right angled, edge position&lt;br&gt;

&lt;br&gt;Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;High current Wire-to-Board &amp; Board-to-Board connections
&lt;br&gt;Angled electrical connection of cable or PCBs
&lt;br&gt;Angled mechanical assembling of PCBs on housings
&lt;br&gt;Suitable for rough environmental conditions

&lt;b&gt;&lt;br&gt;&lt;br&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Bulk

&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature	-55 up to +150 °C
&lt;br&gt;Material	Brass
&lt;br&gt;Surface	Tin
&lt;br&gt;Execution	Press-Fit
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o728011v209%20746221xx_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o728011v209%20746221xx_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/REDCUBE_PRESS-FIT_RIGHT_ANGLED_EDGE_POSITION/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/REDCUBE_PRESS-FIT_RIGHT_ANGLED_EDGE_POSITION&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-12-01&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WP-RAFE"/>
</gates>
<devices>
<device name="_74622103" package="WP-RAFE_74622103">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622103?ae"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="IR" value="130A"/>
<attribute name="PART-NUMBER" value=" 74622103 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="THREAD" value="M3"/>
<attribute name="THREAD-LENGTH" value="4mm"/>
<attribute name="VALUE" value=" 74622103 "/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_74622103_HAL" package="WP-RAFE_74622103_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622103?ae"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="IR" value="130A"/>
<attribute name="PART-NUMBER" value=" 74622103 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="THREAD" value="M3"/>
<attribute name="THREAD-LENGTH" value="4mm"/>
<attribute name="VALUE" value=" 74622103 "/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_74622104" package="WP-RAFE_74622104">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622104?ae"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 74622104 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="THREAD" value="M4"/>
<attribute name="THREAD-LENGTH" value="5mm"/>
<attribute name="VALUE" value=" 74622104 "/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_74622104_HAL" package="WP-RAFE_74622104_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622104?ae"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 74622104 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="THREAD" value="M4"/>
<attribute name="THREAD-LENGTH" value="5mm"/>
<attribute name="VALUE" value=" 74622104 "/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_74622105" package="WP-RAFE_74622105">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622105?ae"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 74622105 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="THREAD" value="M5"/>
<attribute name="THREAD-LENGTH" value="5mm"/>
<attribute name="VALUE" value=" 74622105 "/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_74622105_HAL" package="WP-RAFE_74622105_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622105?ae"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="IR" value="180A"/>
<attribute name="PART-NUMBER" value=" 74622105 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="THREAD" value="M5"/>
<attribute name="THREAD-LENGTH" value="5mm"/>
<attribute name="VALUE" value=" 74622105 "/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_74622106" package="WP-RAFE_74622106">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622106?ae"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="IR" value="250A"/>
<attribute name="PART-NUMBER" value=" 74622106 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="THREAD" value="M6"/>
<attribute name="THREAD-LENGTH" value="8mm"/>
<attribute name="VALUE" value=" 74622106 "/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_74622106_HAL" package="WP-RAFE_74622106_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622106?ae"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="IR" value="250A"/>
<attribute name="PART-NUMBER" value=" 74622106 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="THREAD" value="M6"/>
<attribute name="THREAD-LENGTH" value="8mm"/>
<attribute name="VALUE" value=" 74622106 "/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_74622108_HAL" package="WP-RAFE_74622108_HAL">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622108?ae"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="IR" value="250A"/>
<attribute name="PART-NUMBER" value=" 74622108 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="THREAD" value="M8"/>
<attribute name="THREAD-LENGTH" value="8mm"/>
<attribute name="VALUE" value=" 74622108 "/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_74622108" package="WP-RAFE_74622108">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74622108?ae"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="IR" value="250A"/>
<attribute name="PART-NUMBER" value=" 74622108 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="THREAD" value="M8"/>
<attribute name="THREAD-LENGTH" value="8mm"/>
<attribute name="VALUE" value=" 74622108 "/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
