<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Wire-to-Board Connectors - REDFIT Crimp SKEDD Connector - WR-WSP&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-12-09&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WR-WSP_4911XX014">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="WR-WSP_4911XX015">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="WR-WSP_4911XX012">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="WR-WSP_4911XX013">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 3pins</description>
</package>
<package name="WR-WSP_4911XX011">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 1pins</description>
</package>
</packages>
<symbols>
<symbol name="4P">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3P">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="1P">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="2P">
<description>2Pins Male THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="5P">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="491105014" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491105014?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Black"/>
<attribute name="L" value="28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491105014 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="VALUE" value=" 491105014 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491102014" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491102014?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ White"/>
<attribute name="L" value="28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491102014 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="VALUE" value=" 491102014 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491103014" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491103014?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Blue"/>
<attribute name="L" value="28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491103014 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="VALUE" value=" 491103014 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491104014" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491104014?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Yellow"/>
<attribute name="L" value="28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491104014 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="VALUE" value=" 491104014 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491101014" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491101014?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Red"/>
<attribute name="L" value="28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491101014 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="VALUE" value=" 491101014 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491105012" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491105012?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Black"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491105012 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="VALUE" value=" 491105012 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491101012" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491101012?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Red"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491101012 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="VALUE" value=" 491101012 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491101015" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491101015?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Red"/>
<attribute name="L" value="34mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491101015 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="VALUE" value=" 491101015 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491102015" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491102015?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ White"/>
<attribute name="L" value="34mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491102015 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="VALUE" value=" 491102015 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491103015" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491103015?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Blue"/>
<attribute name="L" value="34mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491103015 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="VALUE" value=" 491103015 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491104015" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491104015?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Yellow"/>
<attribute name="L" value="34mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491104015 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="VALUE" value=" 491104015 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491105015" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491105015?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Black"/>
<attribute name="L" value="34mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491105015 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="VALUE" value=" 491105015 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491103012" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491103012?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Blue"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491103012 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="VALUE" value=" 491103012 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491104012" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491104012?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Yellow"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491104012 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="VALUE" value=" 491104012 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491102012" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491102012?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ White"/>
<attribute name="L" value="16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491102012 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="VALUE" value=" 491102012 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491101013" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491101013?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Red"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491101013 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="VALUE" value=" 491101013 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491103013" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491103013?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Blue"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491103013 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="VALUE" value=" 491103013 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491105011" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491105011?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Black"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491105011 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="VALUE" value=" 491105011 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491102013" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491102013?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ White"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491102013 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="VALUE" value=" 491102013 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491104013" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491104013?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Yellow"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491104013 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="VALUE" value=" 491104013 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491105013" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491105013?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Black"/>
<attribute name="L" value="22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491105013 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="VALUE" value=" 491105013 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491104011" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491104011?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Yellow"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491104011 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="VALUE" value=" 491104011 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491101011" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491101011?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Red"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491101011 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="VALUE" value=" 491101011 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491103011" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491103011?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ Blue"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491103011 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="VALUE" value=" 491103011 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="491102011" prefix="J">
<description>&lt;b&gt;WR-WSP Crimp SKEDD Housing

&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PCB Thickness 1.6 mm  
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Flammability Rating according to UL94 V-0 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;General Information
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Operating Temperature -25 up to +105 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RISO 1000 MΩ 
Withstanding Voltage 1800 V (AC) 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o720451v209%20family-wr-wsp-491101011.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-WSP_CRIMP_SKEDD_HOUSING&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2022-12-09&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1P"/>
</gates>
<devices>
<device name="" package="WR-WSP_4911XX011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/491102011?ae"/>
<attribute name="INSULATOR-COLOR" value="Black/ White"/>
<attribute name="L" value="10mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 491102011 "/>
<attribute name="PINS" value=" 1 "/>
<attribute name="VALUE" value=" 491102011 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
