<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Resistors - Thick Film Resistors - WRIS-KWKB&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Eagle Version 9, Library Revision 2019a, 2019-09-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WRIS-KWKB_1020">
<description>&lt;B&gt;WRIS-KWKB Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;High Power Current Sensing, Wide Terminal
&lt;BR&gt;Size : 1020</description>
</package>
<package name="WRIS-KWKB_0612">
<description>&lt;B&gt;WRIS-KWKB Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;High Power Current Sensing, Wide Terminal
&lt;BR&gt;Size : 0612</description>
</package>
<package name="WRIS-KWKB_1225">
<description>&lt;B&gt;WRIS-KWKB Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;High Power Current Sensing, Wide Terminal
&lt;BR&gt;Size : 1225</description>
</package>
</packages>
<symbols>
<symbol name="R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WRIS-KWKB_0612" prefix="R">
<description>&lt;b&gt;WRIS-KWKB Thick Film Resistors
&lt;br&gt;High Power Current Sensing, Wide Terminal
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for high power current sensing up to 2 W Mounting style: SMT-Chip (wide terminal)
&lt;br&gt;Resistance range: 2.2 Ω ‒ 18 kΩ
&lt;br&gt;Resistance tolerance: ±1 %; ±5 %
&lt;br&gt;Rated Power: 0.75 W ‒ 2W
&lt;br&gt;TCR: ±200 ppm/°C
&lt;br&gt;Operating temperature: -55°C up to +155°C
&lt;br&gt;Sizes: 0612 / 1020 / 1225
&lt;br&gt;Recommended soldering: Reflow soldering
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Electric motor
&lt;br&gt;Camera
&lt;br&gt;Lighting control
&lt;br&gt;TV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135741v209%20Family_WRIS-KWKB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135741v209%20Family_WRIS-KWKB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KWKB"&gt;https://katalog.we-online.com/en/pbs/WRIS-KWKB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="" package="WRIS-KWKB_0612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_561020132004">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132004.pdf"/>
<attribute name="IR" value="126.3mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132004 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB061247R0J304DAATP0000"/>
<attribute name="VALUE" value="47Ohm"/>
</technology>
<technology name="_561020132008">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132008.pdf"/>
<attribute name="IR" value="86600mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132008 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06121000F304DAATP0000"/>
<attribute name="VALUE" value="100Ohm"/>
</technology>
<technology name="_561020132009">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132009.pdf"/>
<attribute name="IR" value="86.6mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132009 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06121000J304DAATP0000"/>
<attribute name="VALUE" value="100Ohm"/>
</technology>
<technology name="_561020132010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132010.pdf"/>
<attribute name="IR" value="82.6mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132010 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06121100J304DAATP0000"/>
<attribute name="VALUE" value="110Ohm"/>
</technology>
<technology name="_561020132011">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132011.pdf"/>
<attribute name="IR" value="79.1mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132011 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06121200F304DAATP0000"/>
<attribute name="VALUE" value="120Ohm"/>
</technology>
<technology name="_561020132014">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132014.pdf"/>
<attribute name="IR" value="55.9mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132014 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06122400F304DAATP0000"/>
<attribute name="VALUE" value="240Ohm"/>
</technology>
<technology name="_561020132023">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132023.pdf"/>
<attribute name="IR" value="39.9mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132023 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06124700J304DAATP0000"/>
<attribute name="VALUE" value="470Ohm"/>
</technology>
<technology name="_561020132030">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132030.pdf"/>
<attribute name="IR" value="25mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132030 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06121201F304DAATP0000"/>
<attribute name="VALUE" value="1200Ohm"/>
</technology>
<technology name="_561020132031">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132031.pdf"/>
<attribute name="IR" value="22.4mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132031 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06121501F304DAATP0000"/>
<attribute name="VALUE" value="1500Ohm"/>
</technology>
<technology name="_561020132032">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132032.pdf"/>
<attribute name="IR" value="20.4mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132032 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06121801F304DAATP0000"/>
<attribute name="VALUE" value="1800Ohm"/>
</technology>
<technology name="_561020132034">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132034.pdf"/>
<attribute name="IR" value="18.5mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132034 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06122201F304DAATP0000"/>
<attribute name="VALUE" value="2200Ohm"/>
</technology>
<technology name="_561020132037">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132037.pdf"/>
<attribute name="IR" value="16.7mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132037 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06122701F304DAATP0000"/>
<attribute name="VALUE" value="2700Ohm"/>
</technology>
<technology name="_561020132059">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020132059.pdf"/>
<attribute name="IR" value="6.5mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020132059 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB06121802F304DAATP0000"/>
<attribute name="VALUE" value="18000Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-KWKB_1020" prefix="R">
<description>&lt;b&gt;WRIS-KWKB Thick Film Resistors
&lt;br&gt;High Power Current Sensing, Wide Terminal
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for high power current sensing up to 2 W Mounting style: SMT-Chip (wide terminal)
&lt;br&gt;Resistance range: 2.2 Ω ‒ 18 kΩ
&lt;br&gt;Resistance tolerance: ±1 %; ±5 %
&lt;br&gt;Rated Power: 0.75 W ‒ 2W
&lt;br&gt;TCR: ±200 ppm/°C
&lt;br&gt;Operating temperature: -55°C up to +155°C
&lt;br&gt;Sizes: 0612 / 1020 / 1225
&lt;br&gt;Recommended soldering: Reflow soldering
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Electric motor
&lt;br&gt;Camera
&lt;br&gt;Lighting control
&lt;br&gt;TV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135741v209%20Family_WRIS-KWKB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135741v209%20Family_WRIS-KWKB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KWKB"&gt;https://katalog.we-online.com/en/pbs/WRIS-KWKB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="" package="WRIS-KWKB_1020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_561020150010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020150010.pdf"/>
<attribute name="IR" value="60.9mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020150010 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB10202700F101DAATE0000"/>
<attribute name="VALUE" value="270Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-KWKB_1225" prefix="R">
<description>&lt;b&gt;WRIS-KWKB Thick Film Resistors
&lt;br&gt;High Power Current Sensing, Wide Terminal
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for high power current sensing up to 2 W Mounting style: SMT-Chip (wide terminal)
&lt;br&gt;Resistance range: 2.2 Ω ‒ 18 kΩ
&lt;br&gt;Resistance tolerance: ±1 %; ±5 %
&lt;br&gt;Rated Power: 0.75 W ‒ 2W
&lt;br&gt;TCR: ±200 ppm/°C
&lt;br&gt;Operating temperature: -55°C up to +155°C
&lt;br&gt;Sizes: 0612 / 1020 / 1225
&lt;br&gt;Recommended soldering: Reflow soldering
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Electric motor
&lt;br&gt;Camera
&lt;br&gt;Lighting control
&lt;br&gt;TV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135741v209%20Family_WRIS-KWKB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135741v209%20Family_WRIS-KWKB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KWKB"&gt;https://katalog.we-online.com/en/pbs/WRIS-KWKB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="" package="WRIS-KWKB_1225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_561020163011">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020163011.pdf"/>
<attribute name="IR" value="86.1mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020163011 "/>
<attribute name="PRATED" value="2W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB12252700F201DAATE0000"/>
<attribute name="VALUE" value="270Ohm"/>
</technology>
<technology name="_561020163012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020163012.pdf"/>
<attribute name="IR" value="68.2mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020163012 "/>
<attribute name="PRATED" value="2W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB12254300J201DAATE0000"/>
<attribute name="VALUE" value="430Ohm"/>
</technology>
<technology name="_561020163016">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020163016.pdf"/>
<attribute name="IR" value="953.5mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020163016 "/>
<attribute name="PRATED" value="2W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB12252R20F201DAATE0000"/>
<attribute name="VALUE" value="2.2Ohm"/>
</technology>
<technology name="_561020163017">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020163017.pdf"/>
<attribute name="IR" value="626.2mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020163017 "/>
<attribute name="PRATED" value="2W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB12255R10F201DAATE0000"/>
<attribute name="VALUE" value="5.1Ohm"/>
</technology>
<technology name="_561020163018">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561020163018.pdf"/>
<attribute name="IR" value="447.2mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561020163018 "/>
<attribute name="PRATED" value="2W"/>
<attribute name="TCR" value="±200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KB122510R0F201DAATE0000"/>
<attribute name="VALUE" value="10Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
