<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Resistors - Thick Film Resistors - WRIS-KWKH&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Eagle Version 9, Library Revision 2019a, 2019-09-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WRIS-KWKH_1020">
<description>&lt;B&gt;WRIS-KWKH Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;High Power Current Sensing, Wide Terminal
&lt;BR&gt;Size : 1020</description>
</package>
<package name="WRIS-KWKH_0612">
<description>&lt;B&gt;WRIS-KWKH Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;High Power Current Sensing, Wide Terminal
&lt;BR&gt;Size : 0612</description>
</package>
</packages>
<symbols>
<symbol name="R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WRIS-KWKH_1020" prefix="R">
<description>&lt;b&gt; WRIS-KWKH Thick Film Resistors
&lt;br&gt;High Power Current Sensing, Wide Terminal
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for high power current sensing up to 1 W Mounting style: SMT-Chip (wide terminal)
&lt;br&gt;Resistance range: 100 mΩ ‒ 620 Ω
&lt;br&gt;Resistance tolerance: ±1% / ±5%
&lt;br&gt;Rated Power: 1 W
&lt;br&gt;TCR: +200; +250; +350 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Sizes: 0612 / 1020
&lt;br&gt;Recommended soldering: Reflow soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Camera
&lt;br&gt;Night vision device
&lt;br&gt;TV
&lt;br&gt;Lighting

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135742v209%20Family_WRIS-KWKH.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135742v209%20Family_WRIS-KWKH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KWKH"&gt;https://katalog.we-online.com/en/pbs/WRIS-KWKH&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="" package="WRIS-KWKH_1020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_561070350055">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070350055.pdf"/>
<attribute name="IR" value="2.58A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070350055 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="350ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH1020R150F101QAATE0000"/>
<attribute name="VALUE" value="0.15Ohm"/>
</technology>
<technology name="_561070350077">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070350077.pdf"/>
<attribute name="IR" value="1.41A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070350077 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH1020R500F101HAATE0000"/>
<attribute name="VALUE" value="0.5Ohm"/>
</technology>
<technology name="_561070350078">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070350078.pdf"/>
<attribute name="IR" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070350078 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH1020R510F101HAATE0000"/>
<attribute name="VALUE" value="0.51Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-KWKH_0612" prefix="R">
<description>&lt;b&gt; WRIS-KWKH Thick Film Resistors
&lt;br&gt;High Power Current Sensing, Wide Terminal
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Product series for high power current sensing up to 1 W Mounting style: SMT-Chip (wide terminal)
&lt;br&gt;Resistance range: 100 mΩ ‒ 620 Ω
&lt;br&gt;Resistance tolerance: ±1% / ±5%
&lt;br&gt;Rated Power: 1 W
&lt;br&gt;TCR: +200; +250; +350 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Sizes: 0612 / 1020
&lt;br&gt;Recommended soldering: Reflow soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Camera
&lt;br&gt;Night vision device
&lt;br&gt;TV
&lt;br&gt;Lighting

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135742v209%20Family_WRIS-KWKH.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135742v209%20Family_WRIS-KWKH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KWKH"&gt;https://katalog.we-online.com/en/pbs/WRIS-KWKH&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-06&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="" package="WRIS-KWKH_0612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_561070332051">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332051.pdf"/>
<attribute name="IR" value="3.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332051 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="350ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R100F101QAATP0000"/>
<attribute name="VALUE" value="100mOhm"/>
</technology>
<technology name="_561070332055">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332055.pdf"/>
<attribute name="IR" value="2.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332055 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="350ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R150F101QAATP0000"/>
<attribute name="VALUE" value="150mOhm"/>
</technology>
<technology name="_561070332057">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332057.pdf"/>
<attribute name="IR" value="2.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332057 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="350ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R180F101QAATP0000"/>
<attribute name="VALUE" value="180mOhm"/>
</technology>
<technology name="_561070332071">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332071.pdf"/>
<attribute name="IR" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332071 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="250ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R330F101LAATP0000"/>
<attribute name="VALUE" value="330mOhm"/>
</technology>
<technology name="_561070332076">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332076.pdf"/>
<attribute name="IR" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332076 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="250ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R470F101LAATP0000"/>
<attribute name="VALUE" value="470mOhm"/>
</technology>
<technology name="_561070332078">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332078.pdf"/>
<attribute name="IR" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332078 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R510F101HAATP0000"/>
<attribute name="VALUE" value="510mOhm"/>
</technology>
<technology name="_561070332079">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332079.pdf"/>
<attribute name="IR" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332079 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R560F101HAATP0000"/>
<attribute name="VALUE" value="560mOhm"/>
</technology>
<technology name="_561070332080">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332080.pdf"/>
<attribute name="IR" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332080 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R600F101HAATP0000"/>
<attribute name="VALUE" value="600mOhm"/>
</technology>
<technology name="_561070332081">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332081.pdf"/>
<attribute name="IR" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332081 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R620F101HAATP0000"/>
<attribute name="VALUE" value="620mOhm"/>
</technology>
<technology name="_561070332092">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332092.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332092 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="250ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R240J101LAATP0000"/>
<attribute name="VALUE" value="240mOhm"/>
</technology>
<technology name="_561070332096">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/561070332096.pdf"/>
<attribute name="IR" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 561070332096 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="250ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KH0612R330J101LAATP0000"/>
<attribute name="VALUE" value="330mOhm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
