<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Active Components - Sensors

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-07-14
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PDXS_VERTICAL">
<description>WSEN-PDXS Differential Pressure Sensor

Vertical-straight nozzles, SMT, 8pins
LXWXH=13.31mmX8mmX7.55mm</description>
</package>
<package name="WSEN-PADS_2511020213301">
<description>WSEN-PADS Absolute Pressure Sensor

SMT, 10pins
LXWXH=2mmX2mmX0.8mm</description>
</package>
<package name="WSEN-ISDS_2536030320001">
<description>WSEN-ISDS 6-axis Inertial Sensor

SMT, 14pins
LXWXH=3mmX2.5mmX0.86MM</description>
</package>
<package name="WE-RCDS_791002002">
<description>WE RCDS Residual Current Detection Sensor 

Vertical, THT 
LXWXH=39.8X13.2X44.9mm</description>
</package>
<package name="WE-PDXS_HORIZONTAL">
<description>WSEN-PDXS Differential Pressure Sensor

Horizontal-barbed nozzles, SMT, 8pins
LXWXH=13.31mmX11.6mmX4.56mm</description>
</package>
<package name="WSEN-ACCE_250028161540X">
<description>WSEN-ACCE Pressure Adapter

250028161540x</description>
</package>
<package name="WE-RCDS_791002004">
<description>WE RCDS Residual Current Detection Sensor 

Horizontal, THT 
LXWXH=30.6X49X16.3mm</description>
</package>
<package name="WSEN-TIDS_2521020222501">
<description>WSEN-TIDS Temperature Sensor IC

SMT, 6pins
LXWXH=2mmX2mmX0.55mm</description>
</package>
<package name="WSEN-ACCE_2500060600000_GLUE">
<description>WSEN-ACCE Filter Cap

Filter Cap - pin holes use for adjusment only
Protection cap for WSEN-HIDS, 5.28 mm spacing
LXWXH=6mmX6mmX3.4mm</description>
</package>
<package name="WSEN-ACCE_2500060600000_PRESSFIT">
<description>WSEN-ACCE Filter Cap

Filter Cap - pin holes for clipping the filter cap on the pcb
Protection cap for WSEN-HIDS, 5.1 mm ± 0.05 mm spacing
LXWXH=6mmX6mmX3.4mm</description>
</package>
<package name="WSEN-HIDS_2525020210002_FILTERCAP_PRESSFIT">
<description>WSEN-HIDS Humidity Sensor with integrated Temperature Sensor
2525020210002, SMT, 4pins
LXWXH=1.5mmX1.5mmX0.54mm

WSEN-ACCE Filter Cap
2500060600000, Protection cap for WSEN-HIDS, 5.1 mm ± 0.05 mm
Use this footprint to use the holes for pressing fit the pins of filter cap into the PCB.
LXWXH=6mmX6mmX3.4mm</description>
</package>
<package name="WSEN-HIDS_2525020210002">
<description>WSEN-HIDS Humidity Sensor with integrated Temperature Sensor

SMT, 4pins
LXWXH=1.5mmX1.5mmX0.54mm
</description>
</package>
<package name="WSEN-HIDS_2525020210002_FILTERCAP_GLUE">
<description>WSEN-HIDS Humidity Sensor with integrated Temperature Sensor
2525020210002, SMT, 4pins
LXWXH=1.5mmX1.5mmX0.54mm

WSEN-ACCE Filter Cap
2500060600000, Protection cap for WSEN-HIDS, 5.28 mm spacing
Use this footprint, if the holes for the pins of the filter cap are used only for adjustment.
LXWXH=6mmX6mmX3.4mm
</description>
</package>
<package name="WSEN-ITDS_2533020201601">
<description>WSEN-ITDS 3 Axis Acceleration Sensor

SMT, 12pins
LXWXH=2mmX2mmX0.7mm</description>
</package>
</packages>
<symbols>
<symbol name="WSEN-PDMS">
<pin name="1" direction="in" function="clk"/>
<pin name="2"/>
<pin name="3" direction="pwr"/>
<pin name="4" direction="out"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6" direction="nc"/>
<pin name="5" direction="pwr"/>
</symbol>
<symbol name="WSEN-PDUS">
<pin name="1" direction="in" function="clk"/>
<pin name="2"/>
<pin name="3" direction="pwr"/>
<pin name="4" direction="out"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6" direction="nc"/>
<pin name="5" direction="pwr"/>
</symbol>
<symbol name="WSEN-PADS_2511020213301">
<pin name="VDD_IO" direction="pwr"/>
<pin name="SCL" direction="in" function="clk"/>
<pin name="RSVD"/>
<pin name="SDA"/>
<pin name="SAO"/>
<pin name="CS" direction="in"/>
<pin name="INT" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="WSEN-ISDS_2536030320001">
<pin name="SA0"/>
<pin name="RSVD@3" direction="pas"/>
<pin name="RSVD@4" direction="pas"/>
<pin name="INT_0" direction="out"/>
<pin name="VDD_IO" direction="pwr"/>
<pin name="GND_2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INT_1" direction="out"/>
<pin name="RSVD@1" direction="pas"/>
<pin name="RSVD@0" direction="pas"/>
<pin name="CS" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
</symbol>
<symbol name="791002002">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WSEN-ACCE_250028161540X">
</symbol>
<symbol name="791002004">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="WSEN-TIDS_2521020222501">
<pin name="SCL"/>
<pin name="INT"/>
<pin name="VDD" direction="pwr"/>
<pin name="SAO"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="P$1"/>
</symbol>
<symbol name="WSEN-ACCE_2500060600000">
</symbol>
<symbol name="WSEN-HIDS_2525020210002">
<pin name="VDD" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WSEN-ITDS_2533020201601">
<pin name="SCL" direction="in" function="clk"/>
<pin name="CS" direction="in"/>
<pin name="SAO"/>
<pin name="SDA"/>
<pin name="NC" direction="nc"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RSVD"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD_IO" direction="pwr"/>
<pin name="INT_1"/>
<pin name="INT_0" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WSEN-PDMS_2513130810305" prefix="IC">
<description>WSEN-PDUS - 2513130810001

5 V, ±0.1kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDMS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130810305"/>
<attribute name="VALUE" value="2513130810305"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810305?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDUS_2513130810201" prefix="IC">
<description>WSEN-PDUS - 2513130810201

5 V, ±10kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDUS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130810201"/>
<attribute name="VALUE" value="2513130810201"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810201?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDMS_2513130810405" prefix="IC">
<description>WSEN-PDUS - 2513130810001

5 V, ±0.1kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDMS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130810405"/>
<attribute name="VALUE" value="2513130810405"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810405?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PADS_25110202133011" prefix="IC">
<description>WSEN-PADS - 2511020213301

Absolute Pressure Sensor

Details see: https://www.we-online.com/katalog/en/WSEN-PADS</description>
<gates>
<gate name="G$1" symbol="WSEN-PADS_2511020213301"/>
</gates>
<devices>
<device name="" package="WSEN-PADS_2511020213301">
<connects>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="INT" pad="7"/>
<connect gate="G$1" pin="RSVD" pad="3"/>
<connect gate="G$1" pin="SAO" pad="5"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="PART-NUMBER" value="25110202133011"/>
<attribute name="VALUE" value="25110202133011"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/25110202133011?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PADS_2511020213301" prefix="IC">
<description>WSEN-PADS - 2511020213301

Absolute Pressure Sensor

Details see: https://www.we-online.com/katalog/en/WSEN-PADS</description>
<gates>
<gate name="G$1" symbol="WSEN-PADS_2511020213301"/>
</gates>
<devices>
<device name="" package="WSEN-PADS_2511020213301">
<connects>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="INT" pad="7"/>
<connect gate="G$1" pin="RSVD" pad="3"/>
<connect gate="G$1" pin="SAO" pad="5"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="PART-NUMBER" value="2511020213301"/>
<attribute name="VALUE" value="2511020213301"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2511020213301?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDUS_2513130810001" prefix="IC">
<description>WSEN-PDUS - 2513130810001

5 V, ±0.1kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDUS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130810001"/>
<attribute name="VALUE" value="2513130810001"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810001?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDUS_2513130815401" prefix="IC">
<description>WSEN-PDUS - 2513130815401

5 V, 0 kPa to 1500 kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDUS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130815401"/>
<attribute name="VALUE" value="2513130815401"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130815401?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDUS_2513130810101" prefix="IC">
<description>WSEN-PDUS - 2513130810101

5 V, ±1kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDUS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130810101"/>
<attribute name="VALUE" value="2513130810101"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810101?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDUS_2513130810401" prefix="IC">
<description>WSEN-PDUS - 2513130810401

5 V, -100 kPa to 1000 kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDUS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130810401"/>
<attribute name="VALUE" value="2513130810401"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810401?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDUS_2513130810301" prefix="IC">
<description>WSEN-PDUS - 2513130810301

5 V, 0 kPa to 100 kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDUS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130810301"/>
<attribute name="VALUE" value="2513130810301"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810301?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDUS_2513130810402" prefix="IC">
<description>WSEN-PDUS - 2513130810402

3.3 V, -100 kPa to 1000 kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDUS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="7.55mm"/>
<attribute name="PART-NUMBER" value="2513130810402"/>
<attribute name="VALUE" value="2513130810402"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810402?ae"/>
<attribute name="VERSION" value="Vertical"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-ISDS_25360303200011" prefix="IC">
<description>WSEN-ISDS 6 Axis IMU (Inertial Measurement Unit)
3-Axis Acceleration Sensor and 3-axis Gyroscope Sensor

Details see: www.we-online.com/en/components/products/WSEN-ISDS</description>
<gates>
<gate name="G$1" symbol="WSEN-ISDS_2536030320001"/>
</gates>
<devices>
<device name="" package="WSEN-ISDS_2536030320001">
<connects>
<connect gate="G$1" pin="CS" pad="12"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND_2" pad="7"/>
<connect gate="G$1" pin="INT_0" pad="4"/>
<connect gate="G$1" pin="INT_1" pad="9"/>
<connect gate="G$1" pin="RSVD@0" pad="11"/>
<connect gate="G$1" pin="RSVD@1" pad="10"/>
<connect gate="G$1" pin="RSVD@3" pad="2"/>
<connect gate="G$1" pin="RSVD@4" pad="3"/>
<connect gate="G$1" pin="SA0" pad="1"/>
<connect gate="G$1" pin="SCL" pad="13"/>
<connect gate="G$1" pin="SDA" pad="14"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VDD_IO" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="0.86mm"/>
<attribute name="PART-NUMBER" value="25360303200011"/>
<attribute name="VALUE" value="25360303200011"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/25360303200011?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RCDS_791002002" prefix="IC">
<description>WE-RCDS Residual Current Detection Sensor

for fault current detection in EV-charging applications 

Characteristics 
Compact design for PCB board mounting 
DC 6mA residual direct current detecting RDC-M-Module for mode 3 EV charging 
System fault indication 
Supply voltage drop monitoring 
Module Software certified according to ANSI/UL 1998, Class 1 
Relevant EMC tests according to IEC 62955: 2018 and EN 60730-1 

Applications 
DC- Residual current detection sensor for stationary EV charging devices
To meet IEC 61851-1 (ensure the disconnection of the supply in case of DC fault)
If the Residual Current Detection Sensor WE-RCDS is to be used in combination with a residual current device RCD type A, this offer is directed exclusively at customers who are authorized to use the patent EP 2 571 128 B3 (valid in Austria, Switzerland/Liechtenstein, Germany, Spain, France, Great Britain and Norway) and the parallel property rights CN 103 001 175 B, US 9,397,494 B2 and DE 10 2011 082 941 A1 or who do not offer, manufacture and distribute within the scope of these property rights.

Details see:  www.we-online.com/en/components/products/WE-RCDS

Created by Ella 2024-03-18
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="791002002"/>
</gates>
<devices>
<device name="" package="WE-RCDS_791002002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="44.9mm"/>
<attribute name="PART-NUMBER" value="791002002"/>
<attribute name="VALUE" value="791002002"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/791002002?ae"/>
<attribute name="VERSION" value="Vertical"/>
<attribute name="TYPE" value="Cable Through Hole"/>
<attribute name="I-RESIDUAL" value="6 mA DC"/>
<attribute name="IP" value="80 / 40 A max."/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-ISDS_2536030320001" prefix="IC">
<description>WSEN-ISDS 6 Axis IMU (Inertial Measurement Unit)
3-Axis Acceleration Sensor and 3-axis Gyroscope Sensor

Details see: www.we-online.com/en/components/products/WSEN-ISDS</description>
<gates>
<gate name="G$1" symbol="WSEN-ISDS_2536030320001"/>
</gates>
<devices>
<device name="" package="WSEN-ISDS_2536030320001">
<connects>
<connect gate="G$1" pin="CS" pad="12"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND_2" pad="7"/>
<connect gate="G$1" pin="INT_0" pad="4"/>
<connect gate="G$1" pin="INT_1" pad="9"/>
<connect gate="G$1" pin="RSVD@0" pad="11"/>
<connect gate="G$1" pin="RSVD@1" pad="10"/>
<connect gate="G$1" pin="RSVD@3" pad="2"/>
<connect gate="G$1" pin="RSVD@4" pad="3"/>
<connect gate="G$1" pin="SA0" pad="1"/>
<connect gate="G$1" pin="SCL" pad="13"/>
<connect gate="G$1" pin="SDA" pad="14"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VDD_IO" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="0.86mm"/>
<attribute name="PART-NUMBER" value="2536030320001"/>
<attribute name="VALUE" value="2536030320001"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2536030320001?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDMS_2513130810105" prefix="IC">
<description>WSEN-PDUS - 2513130810102

3.3 V, ±1kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDMS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_HORIZONTAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="4.56mm"/>
<attribute name="PART-NUMBER" value="2513130810105"/>
<attribute name="VALUE" value="2513130810105"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810105?ae"/>
<attribute name="VERSION" value="Horizontal"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDMS_2513130835205" prefix="IC">
<description>WSEN-PDUS - 2513130810102

3.3 V, ±1kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDMS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_HORIZONTAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="4.56mm"/>
<attribute name="PART-NUMBER" value="2513130835205"/>
<attribute name="VALUE" value="2513130835205"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130835205?ae"/>
<attribute name="VERSION" value="Horizontal"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDUS_2513130810102" prefix="IC">
<description>WSEN-PDUS - 2513130810102

3.3 V, ±1kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDUS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_HORIZONTAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="4.56mm"/>
<attribute name="PART-NUMBER" value="2513130810102"/>
<attribute name="VALUE" value="2513130810102"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810102?ae"/>
<attribute name="VERSION" value="Horizontal"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-PDMS_2513130810205" prefix="IC">
<description>WSEN-PDUS - 2513130810102

3.3 V, ±1kPa Differential Pressure Sensor

Details see: https://www.we-online.com/catalog/en/WSEN-PDUS/</description>
<gates>
<gate name="G$1" symbol="WSEN-PDMS"/>
</gates>
<devices>
<device name="" package="WE-PDXS_HORIZONTAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="4.56mm"/>
<attribute name="PART-NUMBER" value="2513130810205"/>
<attribute name="VALUE" value="2513130810205"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2513130810205?ae"/>
<attribute name="VERSION" value="Horizontal"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-ACCE_250028161540X" prefix="ADAPTER">
<description>WSEN-ACCE Pressure Adapter
250028161540x
</description>
<gates>
<gate name="G$1" symbol="WSEN-ACCE_250028161540X"/>
</gates>
<devices>
<device name="" package="WSEN-ACCE_250028161540X">
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="27.8mm"/>
<attribute name="PART-NUMBER" value="250028161540X"/>
<attribute name="VALUE" value="250028161540X"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RCDS_791002004" prefix="IC">
<description>WE-RCDS Residual Current Detection Sensor

for fault current detection in EV-charging applications 

Characteristics 
Compact design for PCB board mounting 
DC 6mA residual direct current detecting RDC-M-Module for mode 3 EV charging 
System fault indication 
Supply voltage drop monitoring 
Module Software certified according to ANSI/UL 1998, Class 1 
Relevant EMC tests according to IEC 62955: 2018 and EN 60730-1 

Applications 
DC- Residual current detection sensor for stationary EV charging devices
To meet IEC 61851-1 (ensure the disconnection of the supply in case of DC fault)
If the Residual Current Detection Sensor WE-RCDS is to be used in combination with a residual current device RCD type A, this offer is directed exclusively at customers who are authorized to use the patent EP 2 571 128 B3 (valid in Austria, Switzerland/Liechtenstein, Germany, Spain, France, Great Britain and Norway) and the parallel property rights CN 103 001 175 B, US 9,397,494 B2 and DE 10 2011 082 941 A1 or who do not offer, manufacture and distribute within the scope of these property rights.

Details see:  www.we-online.com/en/components/products/WE-RCDS

Created by Ella 2024-03-18
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="791002004"/>
</gates>
<devices>
<device name="" package="WE-RCDS_791002004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="16.3mm"/>
<attribute name="PART-NUMBER" value="791002004"/>
<attribute name="VALUE" value="791002004"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/791002004?ae"/>
<attribute name="VERSION" value="Horizontal"/>
<attribute name="TYPE" value="3-phase primary conductor"/>
<attribute name="I-RESIDUAL" value="6 mA DC"/>
<attribute name="IP" value="40 A max."/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-TIDS_2521020222501" prefix="IC">
<description>WSEN-TIDS Temperature Sensor IC

Details see: www.we-online.com/en/components/products/WSEN-TIDS</description>
<gates>
<gate name="G$1" symbol="WSEN-TIDS_2521020222501"/>
</gates>
<devices>
<device name="" package="WSEN-TIDS_2521020222501">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="INT" pad="2"/>
<connect gate="G$1" pin="P$1" pad="Z1"/>
<connect gate="G$1" pin="SAO" pad="4"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="PART-NUMBER" value="2521020222501"/>
<attribute name="VALUE" value="2521020222501"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2521020222501?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-ACCE_2500060600000" prefix="FC">
<description>WSEN-ACCE filter cap

Protection cap for WSEN-HIDS

Details see: www.we-online.com/en/components/products/WSEN-HIDS</description>
<gates>
<gate name="G$1" symbol="WSEN-ACCE_2500060600000"/>
</gates>
<devices>
<device name="PRESSFIT" package="WSEN-ACCE_2500060600000_PRESSFIT">
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="NR" value="2500060600000"/>
</technology>
</technologies>
</device>
<device name="GLUE" package="WSEN-ACCE_2500060600000_GLUE">
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="PART-NUMBER" value="2500060600000"/>
<attribute name="VALUE" value="2500060600000"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2500060600000?ae"/>
<attribute name="HEIGH" value="1.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-HIDS_2525020210002" prefix="IC">
<description>WSEN-HIDS Humidity Sensor with integrated Temperature Sensor

Details see: www.we-online.com/en/components/products/WSEN-HIDS
</description>
<gates>
<gate name="G$1" symbol="WSEN-HIDS_2525020210002"/>
</gates>
<devices>
<device name="" package="WSEN-HIDS_2525020210002">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="0.54mm"/>
<attribute name="PART-NUMBER" value="2525020210002"/>
<attribute name="VALUE" value="2525020210002"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2525020210002?ae"/>
<attribute name="PROTECTION-CAP" value=" 2500060600000 "/>
</technology>
</technologies>
</device>
<device name="_FILTERCAP_PRESSFIT" package="WSEN-HIDS_2525020210002_FILTERCAP_PRESSFIT">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="PART-NUMBER" value="2525020210002"/>
<attribute name="VALUE" value="2525020210002&amp;2500060600000"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2525020210002?ae"/>
<attribute name="PROTECTION-CAP" value=" 2500060600000 "/>
<attribute name="COMMENT" value="Article numbers for HIDS and filter cap"/>
</technology>
</technologies>
</device>
<device name="_FILTERCAP_GLUE" package="WSEN-HIDS_2525020210002_FILTERCAP_GLUE">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="PART-NUMBER" value="2525020210002"/>
<attribute name="VALUE" value="2525020210002&amp;2500060600000"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2525020210002?ae"/>
<attribute name="PROTECTION-CAP" value=" 2500060600000 "/>
<attribute name="COMMENT" value="Article numbers for HIDS and filter cap"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-ITDS_25330202016011" prefix="IC">
<description>WSEN-ITDS 3 Axis Acceleration Sensor

Details see: www.we-online.com/en/components/products/WSEN-ITDS</description>
<gates>
<gate name="G$1" symbol="WSEN-ITDS_2533020201601"/>
</gates>
<devices>
<device name="" package="WSEN-ITDS_2533020201601">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="INT_0" pad="12"/>
<connect gate="G$1" pin="INT_1" pad="11"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="RSVD" pad="7"/>
<connect gate="G$1" pin="SAO" pad="3"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VDD_IO" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="0.7mm"/>
<attribute name="PART-NUMBER" value="25330202016011"/>
<attribute name="VALUE" value="25330202016011"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/25330202016011?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSEN-ITDS_2533020201601" prefix="IC">
<description>WSEN-ITDS 3 Axis Acceleration Sensor

Details see: www.we-online.com/en/components/products/WSEN-ITDS</description>
<gates>
<gate name="G$1" symbol="WSEN-ITDS_2533020201601"/>
</gates>
<devices>
<device name="" package="WSEN-ITDS_2533020201601">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="INT_0" pad="12"/>
<connect gate="G$1" pin="INT_1" pad="11"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="RSVD" pad="7"/>
<connect gate="G$1" pin="SAO" pad="3"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VDD_IO" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="HEIGHT" value="0.7mm"/>
<attribute name="PART-NUMBER" value="2533020201601"/>
<attribute name="VALUE" value="2533020201601"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/2533020201601?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
