<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Passive Components - Power Magnetics - Unshielded Power Inductors - WE-PD2

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-09-17
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PD2_3521">
<description>WE-PD2 SMD Power Inductor

Size: 3521, SMT, 2pins

LXWXH=3X3.5X2.1mm</description>
</package>
<package name="WE-PD2_1054">
<description>WE-PD2 SMD Power Inductor

Size: 1054, SMT, 2pins

LXWXH=9X10X5.4mm</description>
</package>
<package name="WE-PD2_4532">
<description>WE-PD2 SMD Power Inductor

Size: 4532, SMT, 2pins

LXWXH=4X4.5X3.2mm</description>
</package>
<package name="WE-PD2_5848">
<description>WE-PD2 SMD Power Inductor

Size: 5848, SMT, 2pins

LXWXH=5.2X5.8X4.5mm</description>
</package>
<package name="WE-PD2_7850">
<description>WE-PD2 SMD Power Inductor

Size: 7850, SMT, 2pins

LXWXH=7X7.8X5mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PD2_3521" prefix="L">
<description>WE-PD2 SMT Power Inductor

Characteristics
Open size
Saturation currents up to 14 A
Low tolerances at high inductance values
Operating temperature: –40 °C to +125 °C
Recommended solder profile: Reflow

Applications
Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
Integrated DC/DC converter
Optimal attenuation in MHz frequency range

Details see: www.we-online.com/components/products/WE-PD2

Updated by Ella 2025-03-11
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_3521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447732010">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732010"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="RATED_CURRENT" value="2.55 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3 A"/>
<attribute name="SATURATION_CURRENT" value="3.7 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.05 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="160 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732010?ae"/>
</technology>
<technology name="_7447732015">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732015"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="RATED_CURRENT" value="2.08 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.5 A"/>
<attribute name="SATURATION_CURRENT" value="3.05 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.07 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="130 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732015?ae"/>
</technology>
<technology name="_7447732022">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="RATED_CURRENT" value="1.71 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.2 A"/>
<attribute name="SATURATION_CURRENT" value="2.54 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.09 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="100 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732022?ae"/>
</technology>
<technology name="_7447732033">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="RATED_CURRENT" value="1.39 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.9 A"/>
<attribute name="SATURATION_CURRENT" value="2.09 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.12 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="80 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732033?ae"/>
</technology>
<technology name="_7447732047">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="RATED_CURRENT" value="1.16 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.6 A"/>
<attribute name="SATURATION_CURRENT" value="1.77 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.16 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="70 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732047?ae"/>
</technology>
<technology name="_7447732068">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="RATED_CURRENT" value="0.96 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.4 A"/>
<attribute name="SATURATION_CURRENT" value="1.48 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.21 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="55 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732068?ae"/>
</technology>
<technology name="_7447732110">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732110"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="RATED_CURRENT" value="0.8 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.15 A"/>
<attribute name="SATURATION_CURRENT" value="1.23 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.3 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="45 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732110?ae"/>
</technology>
<technology name="_7447732115">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732115"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="RATED_CURRENT" value="0.64 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.95 A"/>
<attribute name="SATURATION_CURRENT" value="1.01 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.43 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="36 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732115?ae"/>
</technology>
<technology name="_7447732122">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="22 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732122"/>
<attribute name="INDUCTANCE" value="22 uH"/>
<attribute name="RATED_CURRENT" value="0.53 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.7 A"/>
<attribute name="SATURATION_CURRENT" value="0.84 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.7 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="28 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732122?ae"/>
</technology>
<technology name="_7447732133">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="33 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732133"/>
<attribute name="INDUCTANCE" value="33 uH"/>
<attribute name="RATED_CURRENT" value="0.43 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.6 A"/>
<attribute name="SATURATION_CURRENT" value="0.7 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.97 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="24 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732133?ae"/>
</technology>
<technology name="_7447732147">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="47 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732147"/>
<attribute name="INDUCTANCE" value="47 uH"/>
<attribute name="RATED_CURRENT" value="0.36 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.5 A"/>
<attribute name="SATURATION_CURRENT" value="0.59 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.33 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732147?ae"/>
</technology>
<technology name="_7447732168">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="68 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732168"/>
<attribute name="INDUCTANCE" value="68 uH"/>
<attribute name="RATED_CURRENT" value="0.3 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.4 A"/>
<attribute name="SATURATION_CURRENT" value="0.49 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.8 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="16 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732168?ae"/>
</technology>
<technology name="_7447732210">
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="3521"/>
<attribute name="VALUE" value="100 uH"/>
<attribute name="WIDTH" value="3.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447732210"/>
<attribute name="INDUCTANCE" value="100 uH"/>
<attribute name="RATED_CURRENT" value="0.24 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.3 A"/>
<attribute name="SATURATION_CURRENT" value="0.41 A"/>
<attribute name="DC_RESISTANCE_MAX" value="2.8 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="12 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447732210?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_1054" prefix="L">
<description>WE-PD2 SMT Power Inductor

Characteristics
Open size
Saturation currents up to 14 A
Low tolerances at high inductance values
Operating temperature: –40 °C to +125 °C
Recommended solder profile: Reflow

Applications
Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
Integrated DC/DC converter
Optimal attenuation in MHz frequency range

Details see: www.we-online.com/components/products/WE-PD2

Updated by Ella 2026-09-17
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_1054">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744776012">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776012"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="RATED_CURRENT" value="6 A"/>
<attribute name="SATURATION_CURRENT" value="11 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.009 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="110 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776012?ae"/>
</technology>
<technology name="_744776025">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="2.5 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776025"/>
<attribute name="INDUCTANCE" value="2.5 uH"/>
<attribute name="RATED_CURRENT" value="5.3 A"/>
<attribute name="SATURATION_CURRENT" value="8 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.012 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="65 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776025?ae"/>
</technology>
<technology name="_744776033">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="RATED_CURRENT" value="5 A"/>
<attribute name="SATURATION_CURRENT" value="7 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.014 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="45 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776033?ae"/>
</technology>
<technology name="_744776047">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="RATED_CURRENT" value="5 A"/>
<attribute name="SATURATION_CURRENT" value="6 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.017 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="41 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776047?ae"/>
</technology>
<technology name="_744776056">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776056"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="RATED_CURRENT" value="4.8 A"/>
<attribute name="SATURATION_CURRENT" value="5.5 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.019 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="38 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776056?ae"/>
</technology>
<technology name="_744776068">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="RATED_CURRENT" value="4.4 A"/>
<attribute name="SATURATION_CURRENT" value="5 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.022 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="34 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776068?ae"/>
</technology>
<technology name="_744776082">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776082"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="RATED_CURRENT" value="4.2 A"/>
<attribute name="SATURATION_CURRENT" value="4.25 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.026 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776082?ae"/>
</technology>
<technology name="_74477610">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477610"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="RATED_CURRENT" value="2.98 A"/>
<attribute name="SATURATION_CURRENT" value="3.24 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.06 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="24 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477610?ae"/>
</technology>
<technology name="_744776112">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="12 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776112"/>
<attribute name="INDUCTANCE" value="12 uH"/>
<attribute name="RATED_CURRENT" value="2.72 A"/>
<attribute name="SATURATION_CURRENT" value="3.15 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.07 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="23 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776112?ae"/>
</technology>
<technology name="_744776115">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776115"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="RATED_CURRENT" value="2.47 A"/>
<attribute name="SATURATION_CURRENT" value="2.88 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.08 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776115?ae"/>
</technology>
<technology name="_744776118">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="18 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776118"/>
<attribute name="INDUCTANCE" value="18 uH"/>
<attribute name="RATED_CURRENT" value="2.36 A"/>
<attribute name="SATURATION_CURRENT" value="2.43 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.09 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="19 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776118?ae"/>
</technology>
<technology name="_744776122">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="22 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776122"/>
<attribute name="INDUCTANCE" value="22 uH"/>
<attribute name="RATED_CURRENT" value="2.04 A"/>
<attribute name="SATURATION_CURRENT" value="2.07 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.1 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="16 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776122?ae"/>
</technology>
<technology name="_744776127">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="27 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776127"/>
<attribute name="INDUCTANCE" value="27 uH"/>
<attribute name="RATED_CURRENT" value="1.95 A"/>
<attribute name="SATURATION_CURRENT" value="1.98 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.11 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="15 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776127?ae"/>
</technology>
<technology name="_744776133">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="33 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776133"/>
<attribute name="INDUCTANCE" value="33 uH"/>
<attribute name="RATED_CURRENT" value="1.78 A"/>
<attribute name="SATURATION_CURRENT" value="1.89 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.12 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="13 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776133?ae"/>
</technology>
<technology name="_744776139">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="39 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776139"/>
<attribute name="INDUCTANCE" value="39 uH"/>
<attribute name="RATED_CURRENT" value="1.62 A"/>
<attribute name="SATURATION_CURRENT" value="1.8 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.14 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="12 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776139?ae"/>
</technology>
<technology name="_744776147">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="47 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776147"/>
<attribute name="INDUCTANCE" value="47 uH"/>
<attribute name="RATED_CURRENT" value="1.45 A"/>
<attribute name="SATURATION_CURRENT" value="1.62 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.17 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="11 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776147?ae"/>
</technology>
<technology name="_744776156">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="56 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776156"/>
<attribute name="INDUCTANCE" value="56 uH"/>
<attribute name="RATED_CURRENT" value="1.36 A"/>
<attribute name="SATURATION_CURRENT" value="1.53 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.19 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="10 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776156?ae"/>
</technology>
<technology name="_744776168">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="68 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776168"/>
<attribute name="INDUCTANCE" value="68 uH"/>
<attribute name="RATED_CURRENT" value="1.19 A"/>
<attribute name="SATURATION_CURRENT" value="1.49 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.22 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="9 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776168?ae"/>
</technology>
<technology name="_744776182">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="82 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776182"/>
<attribute name="INDUCTANCE" value="82 uH"/>
<attribute name="RATED_CURRENT" value="1.11 A"/>
<attribute name="SATURATION_CURRENT" value="1.17 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.25 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="8 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776182?ae"/>
</technology>
<technology name="_74477620">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="100 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477620"/>
<attribute name="INDUCTANCE" value="100 uH"/>
<attribute name="RATED_CURRENT" value="1.02 A"/>
<attribute name="SATURATION_CURRENT" value="1.1 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.35 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="7.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477620?ae"/>
</technology>
<technology name="_744776212">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="120 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776212"/>
<attribute name="INDUCTANCE" value="120 uH"/>
<attribute name="RATED_CURRENT" value="0.94 A"/>
<attribute name="SATURATION_CURRENT" value="0.99 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.4 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="6.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776212?ae"/>
</technology>
<technology name="_744776215">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="150 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776215"/>
<attribute name="INDUCTANCE" value="150 uH"/>
<attribute name="RATED_CURRENT" value="0.81 A"/>
<attribute name="SATURATION_CURRENT" value="0.9 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.47 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="6 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776215?ae"/>
</technology>
<technology name="_744776218">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="180 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776218"/>
<attribute name="INDUCTANCE" value="180 uH"/>
<attribute name="RATED_CURRENT" value="0.76 A"/>
<attribute name="SATURATION_CURRENT" value="0.78 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.63 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="5.4 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776218?ae"/>
</technology>
<technology name="_744776222">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="220 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776222"/>
<attribute name="INDUCTANCE" value="220 uH"/>
<attribute name="RATED_CURRENT" value="0.67 A"/>
<attribute name="SATURATION_CURRENT" value="0.77 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.73 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776222?ae"/>
</technology>
<technology name="_744776227">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="270 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776227"/>
<attribute name="INDUCTANCE" value="270 uH"/>
<attribute name="RATED_CURRENT" value="0.62 A"/>
<attribute name="SATURATION_CURRENT" value="0.68 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.97 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="4.3 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776227?ae"/>
</technology>
<technology name="_744776233">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="330 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776233"/>
<attribute name="INDUCTANCE" value="330 uH"/>
<attribute name="RATED_CURRENT" value="0.52 A"/>
<attribute name="SATURATION_CURRENT" value="0.59 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.15 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="4.1 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776233?ae"/>
</technology>
<technology name="_744776239">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="390 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776239"/>
<attribute name="INDUCTANCE" value="390 uH"/>
<attribute name="RATED_CURRENT" value="0.49 A"/>
<attribute name="SATURATION_CURRENT" value="0.54 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.3 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="3.9 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776239?ae"/>
</technology>
<technology name="_744776247">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="470 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776247"/>
<attribute name="INDUCTANCE" value="470 uH"/>
<attribute name="RATED_CURRENT" value="0.44 A"/>
<attribute name="SATURATION_CURRENT" value="0.5 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.48 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="3.4 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776247?ae"/>
</technology>
<technology name="_744776256">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="560 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776256"/>
<attribute name="INDUCTANCE" value="560 uH"/>
<attribute name="RATED_CURRENT" value="0.39 A"/>
<attribute name="SATURATION_CURRENT" value="0.47 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.9 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="3 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776256?ae"/>
</technology>
<technology name="_744776260">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="600 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776260"/>
<attribute name="INDUCTANCE" value="600 uH"/>
<attribute name="RATED_CURRENT" value="0.7 A"/>
<attribute name="SATURATION_CURRENT" value="0.6 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.39 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="2.9 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776260?ae"/>
</technology>
<technology name="_744776268">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="680 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776268"/>
<attribute name="INDUCTANCE" value="680 uH"/>
<attribute name="RATED_CURRENT" value="0.36 A"/>
<attribute name="SATURATION_CURRENT" value="0.43 A"/>
<attribute name="DC_RESISTANCE_MAX" value="2.25 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="2.7 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776268?ae"/>
</technology>
<technology name="_744776282">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="820 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776282"/>
<attribute name="INDUCTANCE" value="820 uH"/>
<attribute name="RATED_CURRENT" value="0.32 A"/>
<attribute name="SATURATION_CURRENT" value="0.41 A"/>
<attribute name="DC_RESISTANCE_MAX" value="2.55 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="2.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776282?ae"/>
</technology>
<technology name="_74477630">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="1000 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477630"/>
<attribute name="INDUCTANCE" value="1000 uH"/>
<attribute name="RATED_CURRENT" value="0.32 A"/>
<attribute name="SATURATION_CURRENT" value="0.38 A"/>
<attribute name="DC_RESISTANCE_MAX" value="2.6 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="2.3 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477630?ae"/>
</technology>
<technology name="_744776312">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="1200 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776312"/>
<attribute name="INDUCTANCE" value="1200 uH"/>
<attribute name="RATED_CURRENT" value="0.3 A"/>
<attribute name="SATURATION_CURRENT" value="0.38 A"/>
<attribute name="DC_RESISTANCE_MAX" value="3 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="2.1 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776312?ae"/>
</technology>
<technology name="_744776322">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="2200 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776322"/>
<attribute name="INDUCTANCE" value="2200 uH"/>
<attribute name="RATED_CURRENT" value="0.18 A"/>
<attribute name="SATURATION_CURRENT" value="0.26 A"/>
<attribute name="DC_RESISTANCE_MAX" value="5.3 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="1.4 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776322?ae"/>
</technology>
<technology name="_744776315">
<attribute name="HEIGHT" value="5.4mm"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="1054"/>
<attribute name="VALUE" value="1500 uH"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744776315"/>
<attribute name="INDUCTANCE" value="1500 uH"/>
<attribute name="RATED_CURRENT" value="0.24 A"/>
<attribute name="SATURATION_CURRENT" value="0.31 A"/>
<attribute name="DC_RESISTANCE_MAX" value="3.6 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="1.7 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744776315?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_4532" prefix="L">
<description>WE-PD2 SMT Power Inductor

Characteristics
Open size
Saturation currents up to 14 A
Low tolerances at high inductance values
Operating temperature: –40 °C to +125 °C
Recommended solder profile: Reflow

Applications
Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
Integrated DC/DC converter
Optimal attenuation in MHz frequency range

Details see: www.we-online.com/components/products/WE-PD2

Updated by Ella 2025-03-11
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447730">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7447730"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="RATED_CURRENT" value="4 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.55 A"/>
<attribute name="SATURATION_CURRENT" value="5.72 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.049 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="110 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7447730?ae"/>
</technology>
<technology name="_744773014">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="1.4 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773014"/>
<attribute name="INDUCTANCE" value="1.4 uH"/>
<attribute name="RATED_CURRENT" value="3.4 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.45 A"/>
<attribute name="SATURATION_CURRENT" value="5.04 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.056 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="103 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773014?ae"/>
</technology>
<technology name="_744773018">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773018"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="RATED_CURRENT" value="2.7 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.9 A"/>
<attribute name="SATURATION_CURRENT" value="3.6 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.064 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="95 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773018?ae"/>
</technology>
<technology name="_744773022">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="RATED_CURRENT" value="2.5 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.5 A"/>
<attribute name="SATURATION_CURRENT" value="3.38 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.071 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="85 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773022?ae"/>
</technology>
<technology name="_744773027">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="2.7 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773027"/>
<attribute name="INDUCTANCE" value="2.7 uH"/>
<attribute name="RATED_CURRENT" value="2.25 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.25 A"/>
<attribute name="SATURATION_CURRENT" value="2.97 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.079 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="72 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773027?ae"/>
</technology>
<technology name="_744773033">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="RATED_CURRENT" value="2 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="3.15 A"/>
<attribute name="SATURATION_CURRENT" value="2.88 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.086 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="65 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773033?ae"/>
</technology>
<technology name="_744773039">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="3.9 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773039"/>
<attribute name="INDUCTANCE" value="3.9 uH"/>
<attribute name="RATED_CURRENT" value="1.88 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.7 A"/>
<attribute name="SATURATION_CURRENT" value="2.57 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.094 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="61 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773039?ae"/>
</technology>
<technology name="_744773047">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="RATED_CURRENT" value="1.82 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.6 A"/>
<attribute name="SATURATION_CURRENT" value="2.46 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.11 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="50 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773047?ae"/>
</technology>
<technology name="_744773056">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773056"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="RATED_CURRENT" value="1.58 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.4 A"/>
<attribute name="SATURATION_CURRENT" value="2.43 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.126 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="48 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773056?ae"/>
</technology>
<technology name="_744773068">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="RATED_CURRENT" value="1.54 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="2.3 A"/>
<attribute name="SATURATION_CURRENT" value="2.1 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.131 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="41 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773068?ae"/>
</technology>
<technology name="_744773082">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773082"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="RATED_CURRENT" value="1.5 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.85 A"/>
<attribute name="SATURATION_CURRENT" value="1.8 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.146 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="38 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773082?ae"/>
</technology>
<technology name="_74477310">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477310"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="RATED_CURRENT" value="1.45 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.8 A"/>
<attribute name="SATURATION_CURRENT" value="1.74 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.182 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="37 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477310?ae"/>
</technology>
<technology name="_744773112">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="12 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773112"/>
<attribute name="INDUCTANCE" value="12 uH"/>
<attribute name="RATED_CURRENT" value="1.28 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.55 A"/>
<attribute name="SATURATION_CURRENT" value="1.62 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.21 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="32 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773112?ae"/>
</technology>
<technology name="_744773115">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773115"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="RATED_CURRENT" value="1.2 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.35 A"/>
<attribute name="SATURATION_CURRENT" value="1.46 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.235 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="26 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773115?ae"/>
</technology>
<technology name="_744773118">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="18 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773118"/>
<attribute name="INDUCTANCE" value="18 uH"/>
<attribute name="RATED_CURRENT" value="1.1 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.25 A"/>
<attribute name="SATURATION_CURRENT" value="1.29 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.338 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="23 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773118?ae"/>
</technology>
<technology name="_744773122">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="22 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773122"/>
<attribute name="INDUCTANCE" value="22 uH"/>
<attribute name="RATED_CURRENT" value="1 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.2 A"/>
<attribute name="SATURATION_CURRENT" value="1.22 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.37 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773122?ae"/>
</technology>
<technology name="_744773127">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="27 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773127"/>
<attribute name="INDUCTANCE" value="27 uH"/>
<attribute name="RATED_CURRENT" value="0.94 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1.05 A"/>
<attribute name="SATURATION_CURRENT" value="1 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.522 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="21 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773127?ae"/>
</technology>
<technology name="_744773133">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="33 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773133"/>
<attribute name="INDUCTANCE" value="33 uH"/>
<attribute name="RATED_CURRENT" value="0.86 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="1 A"/>
<attribute name="SATURATION_CURRENT" value="0.9 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.54 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773133?ae"/>
</technology>
<technology name="_744773139">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="39 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773139"/>
<attribute name="INDUCTANCE" value="39 uH"/>
<attribute name="RATED_CURRENT" value="0.77 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.9 A"/>
<attribute name="SATURATION_CURRENT" value="0.87 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.587 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="15 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773139?ae"/>
</technology>
<technology name="_744773147">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="47 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773147"/>
<attribute name="INDUCTANCE" value="47 uH"/>
<attribute name="RATED_CURRENT" value="0.68 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.8 A"/>
<attribute name="SATURATION_CURRENT" value="0.85 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.844 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="17 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773147?ae"/>
</technology>
<technology name="_744773156">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="56 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773156"/>
<attribute name="INDUCTANCE" value="56 uH"/>
<attribute name="RATED_CURRENT" value="0.64 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.7 A"/>
<attribute name="SATURATION_CURRENT" value="0.75 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.937 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="16 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773156?ae"/>
</technology>
<technology name="_744773168">
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4532"/>
<attribute name="VALUE" value="68 uH"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744773168"/>
<attribute name="INDUCTANCE" value="68 uH"/>
<attribute name="RATED_CURRENT" value="0.56 A"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="0.65 A"/>
<attribute name="SATURATION_CURRENT" value="0.68 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.117 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="13 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744773168?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_5848" prefix="L">
<description>WE-PD2 SMT Power Inductor

Characteristics
Open size
Saturation currents up to 14 A
Low tolerances at high inductance values
Operating temperature: –40 °C to +125 °C
Recommended solder profile: Reflow

Applications
Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
Integrated DC/DC converter
Optimal attenuation in MHz frequency range

Details see: www.we-online.com/components/products/WE-PD2

Updated by Ella 2025-03-11
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_5848">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744774022">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774022"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="RATED_CURRENT" value="4.6 A"/>
<attribute name="SATURATION_CURRENT" value="8.2 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.041 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="54 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774022?ae"/>
</technology>
<technology name="_744774027">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="2.7 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774027"/>
<attribute name="INDUCTANCE" value="2.7 uH"/>
<attribute name="RATED_CURRENT" value="4 A"/>
<attribute name="SATURATION_CURRENT" value="8 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.045 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="50 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774027?ae"/>
</technology>
<technology name="_744774033">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774033"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="RATED_CURRENT" value="4 A"/>
<attribute name="SATURATION_CURRENT" value="7.5 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.06 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="43 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774033?ae"/>
</technology>
<technology name="_744774047">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774047"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="RATED_CURRENT" value="3 A"/>
<attribute name="SATURATION_CURRENT" value="5.5 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.071 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="33 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774047?ae"/>
</technology>
<technology name="_744774068">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774068"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="RATED_CURRENT" value="2.4 A"/>
<attribute name="SATURATION_CURRENT" value="5 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.082 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="28 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774068?ae"/>
</technology>
<technology name="_74477410">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477410"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="RATED_CURRENT" value="2.2 A"/>
<attribute name="SATURATION_CURRENT" value="2.5 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.1 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="26 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477410?ae"/>
</technology>
<technology name="_744774112">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="12 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774112"/>
<attribute name="INDUCTANCE" value="12 uH"/>
<attribute name="RATED_CURRENT" value="2 A"/>
<attribute name="SATURATION_CURRENT" value="1.94 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.11 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="24 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774112?ae"/>
</technology>
<technology name="_744774115">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774115"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="RATED_CURRENT" value="1.53 A"/>
<attribute name="SATURATION_CURRENT" value="1.9 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.14 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="23 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774115?ae"/>
</technology>
<technology name="_744774118">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="18 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774118"/>
<attribute name="INDUCTANCE" value="18 uH"/>
<attribute name="RATED_CURRENT" value="1.45 A"/>
<attribute name="SATURATION_CURRENT" value="1.69 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.15 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="21 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774118?ae"/>
</technology>
<technology name="_744774122">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="22 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774122"/>
<attribute name="INDUCTANCE" value="22 uH"/>
<attribute name="RATED_CURRENT" value="1.28 A"/>
<attribute name="SATURATION_CURRENT" value="1.53 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.18 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="16 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774122?ae"/>
</technology>
<technology name="_744774127">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="27 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774127"/>
<attribute name="INDUCTANCE" value="27 uH"/>
<attribute name="RATED_CURRENT" value="1.19 A"/>
<attribute name="SATURATION_CURRENT" value="1.4 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.2 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="15 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774127?ae"/>
</technology>
<technology name="_744774133">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="33 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774133"/>
<attribute name="INDUCTANCE" value="33 uH"/>
<attribute name="RATED_CURRENT" value="1.09 A"/>
<attribute name="SATURATION_CURRENT" value="1.17 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.23 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="14 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774133?ae"/>
</technology>
<technology name="_744774139">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="39 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774139"/>
<attribute name="INDUCTANCE" value="39 uH"/>
<attribute name="RATED_CURRENT" value="0.94 A"/>
<attribute name="SATURATION_CURRENT" value="1.1 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.32 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="12 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774139?ae"/>
</technology>
<technology name="_744774147">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="47 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774147"/>
<attribute name="INDUCTANCE" value="47 uH"/>
<attribute name="RATED_CURRENT" value="0.86 A"/>
<attribute name="SATURATION_CURRENT" value="1 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.37 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="11.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774147?ae"/>
</technology>
<technology name="_744774156">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="56 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774156"/>
<attribute name="INDUCTANCE" value="56 uH"/>
<attribute name="RATED_CURRENT" value="0.77 A"/>
<attribute name="SATURATION_CURRENT" value="0.9 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.42 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="10 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774156?ae"/>
</technology>
<technology name="_744774168">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="68 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774168"/>
<attribute name="INDUCTANCE" value="68 uH"/>
<attribute name="RATED_CURRENT" value="0.64 A"/>
<attribute name="SATURATION_CURRENT" value="0.86 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.46 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="10 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774168?ae"/>
</technology>
<technology name="_744774182">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="82 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774182"/>
<attribute name="INDUCTANCE" value="82 uH"/>
<attribute name="RATED_CURRENT" value="0.6 A"/>
<attribute name="SATURATION_CURRENT" value="0.72 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.6 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="8 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774182?ae"/>
</technology>
<technology name="_74477420">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="100 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477420"/>
<attribute name="INDUCTANCE" value="100 uH"/>
<attribute name="RATED_CURRENT" value="0.57 A"/>
<attribute name="SATURATION_CURRENT" value="0.68 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.65 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="7.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477420?ae"/>
</technology>
<technology name="_744774212">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="120 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774212"/>
<attribute name="INDUCTANCE" value="120 uH"/>
<attribute name="RATED_CURRENT" value="0.49 A"/>
<attribute name="SATURATION_CURRENT" value="0.63 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.93 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="7 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774212?ae"/>
</technology>
<technology name="_744774215">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="150 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774215"/>
<attribute name="INDUCTANCE" value="150 uH"/>
<attribute name="RATED_CURRENT" value="0.46 A"/>
<attribute name="SATURATION_CURRENT" value="0.54 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.1 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="6.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774215?ae"/>
</technology>
<technology name="_744774218">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="180 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774218"/>
<attribute name="INDUCTANCE" value="180 uH"/>
<attribute name="RATED_CURRENT" value="0.42 A"/>
<attribute name="SATURATION_CURRENT" value="0.5 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.38 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="5.8 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774218?ae"/>
</technology>
<technology name="_744774222">
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="LENGTH" value="5.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5848"/>
<attribute name="VALUE" value="220 uH"/>
<attribute name="WIDTH" value="5.8mm"/>
<attribute name="MATERIAL" value="NiZn"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744774222"/>
<attribute name="INDUCTANCE" value="220 uH"/>
<attribute name="RATED_CURRENT" value="0.42 A"/>
<attribute name="SATURATION_CURRENT" value="0.47 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.57 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744774222?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_7850" prefix="L">
<description>WE-PD2 SMT Power Inductor

Characteristics
Open size
Saturation currents up to 14 A
Low tolerances at high inductance values
Operating temperature: –40 °C to +125 °C
Recommended solder profile: Reflow

Applications
Switching regulators with low operating voltages (graphic cards, embedded PC-Cards, mainboards)
Integrated DC/DC converter
Optimal attenuation in MHz frequency range

Details see: www.we-online.com/components/products/WE-PD2

Updated by Ella 2025-03-11
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD2_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74477510">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="10 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477510"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="RATED_CURRENT" value="2.3 A"/>
<attribute name="SATURATION_CURRENT" value="2.95 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.07 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="28 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477510?ae"/>
</technology>
<technology name="_744775112">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="12 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775112"/>
<attribute name="INDUCTANCE" value="12 uH"/>
<attribute name="RATED_CURRENT" value="2.18 A"/>
<attribute name="SATURATION_CURRENT" value="2.2 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.08 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="26 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775112?ae"/>
</technology>
<technology name="_744775115">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="15 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775115"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="RATED_CURRENT" value="1.93 A"/>
<attribute name="SATURATION_CURRENT" value="2.23 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.09 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775115?ae"/>
</technology>
<technology name="_744775118">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="18 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775118"/>
<attribute name="INDUCTANCE" value="18 uH"/>
<attribute name="RATED_CURRENT" value="1.89 A"/>
<attribute name="SATURATION_CURRENT" value="2.14 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.1 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="19 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775118?ae"/>
</technology>
<technology name="_744775122">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="22 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775122"/>
<attribute name="INDUCTANCE" value="22 uH"/>
<attribute name="RATED_CURRENT" value="1.76 A"/>
<attribute name="SATURATION_CURRENT" value="1.81 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.11 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="17.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775122?ae"/>
</technology>
<technology name="_744775127">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="27 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775127"/>
<attribute name="INDUCTANCE" value="27 uH"/>
<attribute name="RATED_CURRENT" value="1.48 A"/>
<attribute name="SATURATION_CURRENT" value="1.62 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.12 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="15.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775127?ae"/>
</technology>
<technology name="_744775133">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="33 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775133"/>
<attribute name="INDUCTANCE" value="33 uH"/>
<attribute name="RATED_CURRENT" value="1.35 A"/>
<attribute name="SATURATION_CURRENT" value="1.47 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.13 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="14.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775133?ae"/>
</technology>
<technology name="_744775139">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="39 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775139"/>
<attribute name="INDUCTANCE" value="39 uH"/>
<attribute name="RATED_CURRENT" value="1.25 A"/>
<attribute name="SATURATION_CURRENT" value="1.33 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.16 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="12.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775139?ae"/>
</technology>
<technology name="_744775147">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="47 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775147"/>
<attribute name="INDUCTANCE" value="47 uH"/>
<attribute name="RATED_CURRENT" value="1.17 A"/>
<attribute name="SATURATION_CURRENT" value="1.24 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.18 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="12 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775147?ae"/>
</technology>
<technology name="_744775156">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="56 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775156"/>
<attribute name="INDUCTANCE" value="56 uH"/>
<attribute name="RATED_CURRENT" value="1.04 A"/>
<attribute name="SATURATION_CURRENT" value="1.14 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.24 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="10.5 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775156?ae"/>
</technology>
<technology name="_744775168">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="68 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775168"/>
<attribute name="INDUCTANCE" value="68 uH"/>
<attribute name="RATED_CURRENT" value="0.99 A"/>
<attribute name="SATURATION_CURRENT" value="1.05 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.28 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="9.7 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775168?ae"/>
</technology>
<technology name="_744775182">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="82 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775182"/>
<attribute name="INDUCTANCE" value="82 uH"/>
<attribute name="RATED_CURRENT" value="0.9 A"/>
<attribute name="SATURATION_CURRENT" value="0.95 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.37 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="8.6 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775182?ae"/>
</technology>
<technology name="_74477520">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="100 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477520"/>
<attribute name="INDUCTANCE" value="100 uH"/>
<attribute name="RATED_CURRENT" value="0.77 A"/>
<attribute name="SATURATION_CURRENT" value="0.86 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.43 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="8 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477520?ae"/>
</technology>
<technology name="_744775210">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="120 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775210"/>
<attribute name="INDUCTANCE" value="120 uH"/>
<attribute name="RATED_CURRENT" value="0.67 A"/>
<attribute name="SATURATION_CURRENT" value="0.81 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.47 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="7 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775210?ae"/>
</technology>
<technology name="_744775215">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="150 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775215"/>
<attribute name="INDUCTANCE" value="150 uH"/>
<attribute name="RATED_CURRENT" value="0.6 A"/>
<attribute name="SATURATION_CURRENT" value="0.71 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.64 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="6.2 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775215?ae"/>
</technology>
<technology name="_744775218">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="180 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775218"/>
<attribute name="INDUCTANCE" value="180 uH"/>
<attribute name="RATED_CURRENT" value="0.55 A"/>
<attribute name="SATURATION_CURRENT" value="0.57 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.71 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="5.8 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775218?ae"/>
</technology>
<technology name="_744775222">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="220 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775222"/>
<attribute name="INDUCTANCE" value="220 uH"/>
<attribute name="RATED_CURRENT" value="0.51 A"/>
<attribute name="SATURATION_CURRENT" value="0.56 A"/>
<attribute name="DC_RESISTANCE_MAX" value="0.96 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="5.4 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775222?ae"/>
</technology>
<technology name="_744775227">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="270 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775227"/>
<attribute name="INDUCTANCE" value="270 uH"/>
<attribute name="RATED_CURRENT" value="0.47 A"/>
<attribute name="SATURATION_CURRENT" value="0.51 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.11 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="4.7 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775227?ae"/>
</technology>
<technology name="_744775233">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="330 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775233"/>
<attribute name="INDUCTANCE" value="330 uH"/>
<attribute name="RATED_CURRENT" value="0.43 A"/>
<attribute name="SATURATION_CURRENT" value="0.48 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.26 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="4.2 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775233?ae"/>
</technology>
<technology name="_744775239">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="390 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775239"/>
<attribute name="INDUCTANCE" value="390 uH"/>
<attribute name="RATED_CURRENT" value="0.38 A"/>
<attribute name="SATURATION_CURRENT" value="0.43 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.77 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="3.9 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775239?ae"/>
</technology>
<technology name="_744775247">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="470 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="744775247"/>
<attribute name="INDUCTANCE" value="470 uH"/>
<attribute name="RATED_CURRENT" value="0.36 A"/>
<attribute name="SATURATION_CURRENT" value="0.38 A"/>
<attribute name="DC_RESISTANCE_MAX" value="1.96 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="3.4 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/744775247?ae"/>
</technology>
<technology name="_74477530">
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="7850"/>
<attribute name="VALUE" value="1000 uH"/>
<attribute name="WIDTH" value="7.8mm"/>
<attribute name="MATERIAL" value="-"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74477530"/>
<attribute name="INDUCTANCE" value="1000 uH"/>
<attribute name="RATED_CURRENT" value="0.3 A"/>
<attribute name="SATURATION_CURRENT" value="0.3 A"/>
<attribute name="DC_RESISTANCE_MAX" value="3.3 ohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="2.4 MHz"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74477530?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
